#	$Id: printer,v 1.1.1.1 1999/02/18 20:05:35 andreas Exp $

Supported printers by Ghostscript and apsfilter
===============================================

[ Version dependent -- Ghostscript 2.6.1 PL 4 supports ]


*	appledmp  Apple Dot Matrix Printer (should also work with Imagewriter)
	bj10e	  Canon BubbleJet BJ10e
*	bj200	  Canon BubbleJet BJ200
*	cdeskjet  H-P DeskJet 500C with 1 bit/pixel color
*	cdjcolor  H-P DeskJet 500C with 24 bit/pixel color and
		      high-quality color (Floyd-Steinberg) dithering
*	cdjmono   H-P DeskJet 500C printing black only
*	cdj500	  H-P DeskJet 500C (same as cdjcolor)
*	cdj550	  H-P DeskJet 550C
*	declj250  alternate DEC LJ250 driver
+	deskjet   H-P DeskJet and DeskJet Plus
*	dfaxhigh  DigiBoard, Inc.'s DigiFAX software format (high resolution)
*	dfaxlow   DigiFAX low (normal) resolution
	djet500   H-P DeskJet 500
*	djet500c  H-P DeskJet 500C
	epson	  Epson-compatible dot matrix printers (9- or 24-pin)
+	eps9high  Epson-compatible 9-pin, interleaved lines
		       (triple resolution)
*	epsonc	  Epson LQ-2550 and Fujitsu 3400/2400/1200 color printers
*	escp2	  Epson ESC/P 2 language printers, including Stylus 800
+	ibmpro    IBM 9-pin Proprinter
*	jetp3852  IBM Jetprinter ink-jet color printer (Model #3852)
+	laserjet  H-P LaserJet
*	la50	  DEC LA50 printer
*	la75	  DEC LA75 printer
*	lbp8	  Canon LBP-8II laser printer
*	ln03	  DEC LN03 printer
*	lj250	  DEC LJ250 Companion color printer
+	ljet2p	  H-P LaserJet IId/IIp/III* with TIFF compression
+	ljet3	  H-P LaserJet III* with Delta Row compression
+	ljet4	  H-P LaserJet 4 (defaults to 600 dpi)
+	ljet4l	  H-P LaserJet 4L (defaults to 300 dpi)
+	ljetplus  H-P LaserJet Plus
*	m8510	  C.Itoh M8510 printer
*	necp6	  NEC P6/P6+/P60 printers at 360 x 360 DPI resolution
*	nwp533    Sony Microsystems NWP533 laser printer   [Sony only]
*	oki182	  Okidata MicroLine 182
	paintjet  H-P PaintJet color printer
*	pj	  alternate PaintJet XL driver 
*	pjxl	  H-P PaintJet XL color printer
*	pjxl300   H-P PaintJet XL300 color printer
*	r4081	  Ricoh 4081 laser printer
*	sparc	  SPARCprinter
*	t4693d2   Tektronix 4693d color printer, 2 bits per R/G/B component
*	t4693d4   Tektronix 4693d color printer, 4 bits per R/G/B component
*	t4693d8   Tektronix 4693d color printer, 8 bits per R/G/B component
*	tek4696   Tektronix 4695/4696 inkjet plotter


Look into the filter directory, if a suitable filter file
(a suitable symblic link to ../bin/apsfilter) is present.

If not, then take a look into bin/mksymlinks, to create the
filter for you. You certainly have to edit this file by hand
before executing it as root ...

See the comments in the script !

New: Support for real Postscript Printer (skips gs(1)) !!!

Printer are named:

	PS_300dpi PS_400dpi PS_600dpi PS_800dpi

