/*****************************************************************************/

/*
 *	istallion.h  -- stallion intelligent multiport serial driver.
 *
 *	Copyright (C) 1996-1998  Stallion Technologies (support@stallion.oz.au).
 *	Copyright (C) 1994-1996  Greg Ungerer (gerg@stallion.oz.au).
 *
 *	This program is free software; you can redistribute it and/or modify
 *	it under the terms of the GNU General Public License as published by
 *	the Free Software Foundation; either version 2 of the License, or
 *	(at your option) any later version.
 *
 *	This program is distributed in the hope that it will be useful,
 *	but WITHOUT ANY WARRANTY; without even the implied warranty of
 *	MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *	GNU General Public License for more details.
 *
 *	You should have received a copy of the GNU General Public License
 *	along with this program; if not, write to the Free Software
 *	Foundation, Inc., 675 Mass Ave, Cambridge, MA 02139, USA.
 */

/*****************************************************************************/
#ifndef	_ISTALLION_H
#define	_ISTALLION_H
/*****************************************************************************/

/*
 *	Define important driver constants here.
 */
#define	STL_MAXBRDS		4
#define	STL_MAXPANELS		4
#define	STL_MAXPORTS		64
#define	STL_MAXCHANS		(STL_MAXPORTS + 1)
#define	STL_MAXDEVS		(STL_MAXBRDS * STL_MAXPORTS)


/*
 *	Define a set of structures to hold all the board/panel/port info
 *	for our ports. These will be dynamically allocated as required at
 *	driver initialization time.
 */

/*
 *	Port and board structures to hold status info about each object.
 *	The board structure contains pointers to structures for each port
 *	connected to it. Panels are not distinguished here, since
 *	communication with the slave board will always be on a per port
 *	basis.
 */
typedef struct {
	unsigned long		magic;
	int			portnr;
	int			panelnr;
	int			brdnr;
	unsigned long		state;
	int			devnr;
	int			flags;
	int			baud_base;
	int			custom_divisor;
	int			close_delay;
	int			closing_wait;
	int			refcount;
	int			openwaitcnt;
	int			rc;
	int			argsize;
	void			*argp;
	long			session;
	long			pgrp;
	unsigned int		rxmarkmsk;
	struct tty_struct	*tty;
	struct wait_queue	*open_wait;
	struct wait_queue	*close_wait;
	struct wait_queue	*raw_wait;
	struct tq_struct	tqhangup;
	struct termios		normaltermios;
	struct termios		callouttermios;
	asysigs_t		asig;
	unsigned long		addr;
	unsigned long		rxoffset;
	unsigned long		txoffset;
	unsigned long		sigs;
	unsigned long		pflag;
	unsigned int		rxsize;
	unsigned int		txsize;
	unsigned char		reqbit;
	unsigned char		portidx;
	unsigned char		portbit;
} stliport_t;

/*
 *	Use a structure of function pointers to do board level operations.
 *	These include, enable/disable, paging shared memory, interrupting, etc.
 */
typedef struct stlibrd {
	unsigned long	magic;
	int		brdnr;
	int		brdtype;
	int		state;
	int		nrpanels;
	int		nrports;
	int		nrdevs;
	unsigned int	iobase;
	int		iosize;
	unsigned long	memaddr;
	void		*membase;
	int		memsize;
	int		pagesize;
	int		hostoffset;
	int		slaveoffset;
	int		bitsize;
	int		enabval;
	int		panels[STL_MAXPANELS];
	int		panelids[STL_MAXPANELS];
	void		(*init)(struct stlibrd *brdp);
	void		(*enable)(struct stlibrd *brdp);
	void		(*reenable)(struct stlibrd *brdp);
	void		(*disable)(struct stlibrd *brdp);
	char		*(*getmemptr)(struct stlibrd *brdp, unsigned long offset, int line);
	void		(*intr)(struct stlibrd *brdp);
	void		(*reset)(struct stlibrd *brdp);
	stliport_t	*ports[STL_MAXPORTS];
} stlibrd_t;


/*
 *	Define MAGIC numbers used for above structures.
 */
#define	STLI_PORTMAGIC	0xe671c7a1
#define	STLI_BOARDMAGIC	0x4bc6c825

/*****************************************************************************/
#endif
