# /etc/bootptab: database for bootp server (/etc/bootpd)
# Last update: gwr, Sun Dec 12 19:00:00 EDT 1993
# Dynamic Examples: al, Sat, Apr 15 12:00:00 EDT 1994
# Blank lines and lines beginning with '#' are ignored.
#
# Legend:	(see bootptab.5)
#	first field -- hostname (not indented)
#	bf -- bootfile
#	bs -- bootfile size in 512-octet blocks
#	cs -- cookie servers
#	df -- dump file name
#	dn -- domain name
#	ds -- domain name servers
#	ef -- extension file
#	gw -- gateways
#	ha -- hardware address
#	hd -- home directory for bootfiles
#	hn -- host name set for client
#	ht -- hardware type
#	im -- impress servers
#	ip -- host IP address
#	lg -- log servers
#	lp -- LPR servers
#	ns -- IEN-116 name servers
#	ra -- reply address
#	rl -- resource location protocol servers
#	rp -- root path
#	sa -- boot server address
#	sm -- subnet mask
#	sw -- swap server
#	tc -- template host (points to similar host entry)
#	td -- TFTP directory
#	to -- time offset (seconds)
#	ts -- time servers
#	vm -- vendor magic number
#	Tn -- generic option tag n
#
# Be careful about including backslashes where they're needed.  Weird (bad)
# things can happen when a backslash is omitted where one is intended.
# Also, note that generic option data must be either a string or a
# sequence of bytes where each byte is a two-digit hex value.

# Dynamic hosts will be added at end of file
# You need to define ranges of dynamic IP to assign from this bootp server
# use dummy name ".dynamic-X" where X is the range number starting with 1
# Generic option tag T254 tells how many IP addresses to assign from that range
# WARNING: don't assign beyond the Class C boundary (or your subnet),
# start a new range

#Examples: including what to add with T250 line
#.dynamic-1:ip=204.213.190.10:T254=0x64:T253=0x02:\
	:T250="gw=204.213.190.1:ds=204.213.176.1":

# How to do part of a class B
#.dynamic-1:ip=137.49.41.1:T254=0xFE:
#.dynamic-2:ip=137.49.42.1:T254=0xFE:
#.dynamic-3:ip=137.49.43.1:T254=0xFE:
#.dynamic-4:ip=137.49.44.1:T254=0xFE:

