<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Supported chipsets </TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="tseng.html"><EM> Information for Tseng Chipset Users</EM></A>
 <b>:</b> <EM>Supported chipsets </EM><BR>
<b>Previous:</b> <A HREF="tseng.html"><EM> Information for Tseng Chipset Users</EM></A><BR>
<b>Next:</b> <A HREF="tseng2.html"><EM>Terminology </EM></A>


<HR NOSHADE>
  <H2><A NAME="1"></A>1. Supported chipsets </H2>

<p>The Tseng chipsets supported by XFree86 are ET3000, ET4000, ET4000/W32 and
ET6000. Accelerated features of the ET4000/W32, W32i, W32p and ET6000 are
supported by the SVGA driver. For details about the separate accelerated
8bpp (=256 color) ET4000/W32 and ET6000 server, refer to
<A href="W32.html">README.W32</A>.</p>
<p>Note that you should NOT be using XF86_W32 unless XF86_SVGA doesn't work on
your hardware. No further development is being done on the W32 server; all
new efforts go into the SVGA server.</p>
<p>Some ET4000W32 ISA cards are known NOT to work with the SVGA server in this
version (XFree86 3.3.1): they hang the machine... Use the W32 server
<code>XF86_W32</code> for these cards!</p>

 <HR NOSHADE>
<A HREF="tseng.html"><EM> Information for Tseng Chipset Users</EM></A>
 <b>:</b> <EM>Supported chipsets </EM><BR>
<b>Previous:</b> <A HREF="tseng.html"><EM> Information for Tseng Chipset Users</EM></A><BR>
<b>Next:</b> <A HREF="tseng2.html"><EM>Terminology </EM></A>



</BODY>
</HTML>
