<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>How Video Displays Work</TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="VideoModes.html"><EM>XFree86 Video Timings HOWTO</EM></A>
 <b>:</b> <EM>How Video Displays Work</EM><BR>
<b>Previous:</b> <A HREF="VideoModes2.html"><EM>Introduction</EM></A><BR>
<b>Next:</b> <A HREF="VideoModes4.html"><EM>Basic Things to Know about your Display and Adapter</EM></A>


<HR NOSHADE>
  <H2><A NAME="3"></A>3. How Video Displays Work<A NAME="video"></A></H2>

<p>Knowing how the display works is essential to understanding what numbers to put
in the various fields in the file Xconfig.  Those values are used in the lowest
levels of controlling the display by the XFree86 server. </p>
<p>The display generates a picture from a series of dots.  The dots are arranged
from left to right to form lines.  The lines are arranged from top to bottom to
form the picture.  The dots emit light when they are struck by the electron
beam inside the display.  To make the beam strike each dot for an equal amount
of time, the beam is swept across the display in a constant pattern. </p>
<p>The pattern starts at the top left of the screen, goes across the screen to the
right in a straight line, and stops temporarily on the right side of the
screen.  Then the beam is swept back to the left side of the display, but down
one line.  The new line is swept from left to right just as the first line was.
This pattern is repeated until the bottom line on the display has been swept.
Then the beam is moved from the bottom right corner of the display to the top
left corner, and the pattern is started over again. </p>
<p>There is one variation of this scheme known as interlacing: here only
every second line is swept during one half-frame and the others are filled in
in during a second half-frame.</p>
<p>Starting the beam at the top left of the display is called the beginning of a
frame.  The frame ends when the beam reaches the the top left corner again as
it comes from the bottom right corner of the display.  A frame is made up of
all of the lines the beam traced from the top of the display to the bottom. </p>
<p>If the electron beam were on all of the time it was sweeping through the frame,
all of the dots on the display would be illuminated.  There would be no black
border around the edges of the display.  At the edges of the display the
picture would become distorted because the beam is hard to control there.  To
reduce the distortion, the dots around the edges of the display are not
illuminated by the beam even though the beam may be pointing at them.  The
viewable area of the display is reduced this way. </p>
<p>Another important thing to understand is what becomes of the beam when no spot
is being painted on the visible area.  The time the beam would have been
illuminating the side borders of the display is used for sweeping the beam back
from the right edge to the left and moving the beam down to the next line.  The
time the beam would have been illuminating the top and bottom borders of the
display is used for moving the beam from the bottom-right corner of the display
to the top-left corner. </p>
<p>The adapter card generates the signals which cause the display to turn on the
electron beam at each dot to generate a picture.  The card also controls when
the display moves the beam from the right side to the left and down a line by
generating a signal called the horizontal sync (for synchronization) pulse.
One horizontal sync pulse occurs at the end of every line.  The adapter also
generates a vertical sync pulse which signals the display to move the beam to
the top-left corner of the display.  A vertical sync pulse is generated near
the end of every frame. </p>
<p>The display requires that there be short time periods both before and after the
horizontal and vertical sync pulses so that the position of the electron beam
can stabilize.  If the beam can't stabilize, the picture will not be steady. </p>
<p>In a later section, we'll come back to these basics with definitions,
formulas and examples to help you use them. </p>

 <HR NOSHADE>
<A HREF="VideoModes.html"><EM>XFree86 Video Timings HOWTO</EM></A>
 <b>:</b> <EM>How Video Displays Work</EM><BR>
<b>Previous:</b> <A HREF="VideoModes2.html"><EM>Introduction</EM></A><BR>
<b>Next:</b> <A HREF="VideoModes4.html"><EM>Basic Things to Know about your Display and Adapter</EM></A>



</BODY>
</HTML>
