<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Configuration:</TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="I128.html"><EM>Information for Number Nine I128 Users</EM></A>
 <b>:</b> <EM>Configuration:</EM><BR>
<b>Previous:</b> <A HREF="I1282.html"><EM>Features:</EM></A><BR>
<b>Next:</b> <A HREF="I1284.html"><EM>Mode lines for the SiliconGraphics flat panel display:</EM></A>


<HR NOSHADE>
  <H2><A NAME="3"></A>3. Configuration:</H2>
<p>The I128 driver should auto-detect all supported hardware so you needn't 
have anything other than the Identifier in the Section "Device" of the
XF86Config file.  When running the XF86Setup or xf86config programs one    
merely needs to select an I128 card so that the correct server will be  
used.  One need not and should not specify a RAMDAC, clockchip or allow 
the setup program to probe for clocks. The driver will auto-detect the   
amount of video ram present.</p>
<p>The following Section "Device" options are supported by the MGA driver:
<ul>
<li>Option "dac_8_bit"
<p>Will enable 8-bit DAC support.</p>
</li>
<li>Option "no_accel"
<p>Will disable all hardware acceleration.</p>
</li>
<li>Option "sync_on_green"
<p>Will enable syncing on green for sync-on-green monitors (these are typically
fixed frequency workstation monitors).</p>
</li>
</ul>
</p>

 <HR NOSHADE>
<A HREF="I128.html"><EM>Information for Number Nine I128 Users</EM></A>
 <b>:</b> <EM>Configuration:</EM><BR>
<b>Previous:</b> <A HREF="I1282.html"><EM>Features:</EM></A><BR>
<b>Next:</b> <A HREF="I1284.html"><EM>Mode lines for the SiliconGraphics flat panel display:</EM></A>



</BODY>
</HTML>
