<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>General Notes </TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="epson.html"><EM> Information for EPSON SPC8110 Users</EM></A>
 <b>:</b> <EM>General Notes </EM><BR>
<b>Previous:</b> <A HREF="epson.html"><EM> Information for EPSON SPC8110 Users</EM></A><BR>
<b>Next:</b> <A HREF="epson2.html"><EM><code>XF86Config</code> options </EM></A>


<HR NOSHADE>
  <H2><A NAME="1"></A>1. General Notes </H2>

<p>This server provides support for the Seiko/EPSON SPC8110F0A LCD VGA
controller chip.</p>
<p>The driver was developed and tested using an EPSON 486D4 CardPC
using CRT display mode. LCD operation was successfully tested
using an earlier release of this driver.</p>
<p>The current driver has support for linear mapping of the frame buffer,
supports the hardware cursor and uses the Bitblt engine for basic
operations such as CopyArea and solid fills.</p>

 <HR NOSHADE>
<A HREF="epson.html"><EM> Information for EPSON SPC8110 Users</EM></A>
 <b>:</b> <EM>General Notes </EM><BR>
<b>Previous:</b> <A HREF="epson.html"><EM> Information for EPSON SPC8110 Users</EM></A><BR>
<b>Next:</b> <A HREF="epson2.html"><EM><code>XF86Config</code> options </EM></A>



</BODY>
</HTML>
