<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Video modes </TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="epson.html"><EM> Information for EPSON SPC8110 Users</EM></A>
 <b>:</b> <EM>Video modes </EM><BR>
<b>Previous:</b> <A HREF="epson2.html"><EM><code>XF86Config</code> options </EM></A><BR>
<b>Next:</b> <A HREF="epson4.html"><EM>Acknowledgments </EM></A>


<HR NOSHADE>
  <H2><A NAME="3"></A>3. Video modes </H2>

<p>The driver probes wether the chip is configured for CRT only or
LCD/simultaneous mode of operation. In the former case it will
enable clock programming and will support any mode which is
within the limits of the hardware. If the chip is configured for
LCD/simultaneous operation mode the driver will respect the
settings of the BIOS and allow only one video mode conforming
with the panel size.</p>
<p>The driver does not support interlaced or double scan modes.</p>

<H3><A NAME="4"></A>3.1. Clocks </H3>

<p>Probing is supported, but of course the usual warnings and
disclaimers apply. Probing may momentarily subject your
monitor/panel to sweep frequencies in excess of its rating.  The
cautious may wish to turn off the monitor while the probe is
running. In CRT mode the driver may produce video timings
inadequate for your monitor, handle with care!</p>
<p>As with many integrated designs the speed of the graphics operations
depend very much of the refresh rate you use. Higher refresh rates
yield lower performance.</p>

<H3><A NAME="5"></A>3.2. Example Modes </H3>

<p>The following XF86Config "Device" section should work for all
configurations:</p>
<p>
<pre>
  Section "Device"
      Identifier "CardPC"
      VendorName "EPSON"
      BoardName  "CardPC"
      Chipset    "spc8110"
      Option    "sw_cursor"
      Membase   0x03e00000
      Option    "no_linear"
      Option    "noaccel"
      Option    "fifo_moderate"
  EndSection
</pre>
</p>
<p>This Modeline was tested in a 640x480 panel configuration:
<pre>
  Modeline "640x480" 28.36   640 672 768 800  480 490 492 525
</pre>
</p>

<p>These Modelines were tested in a CRT configuration:
<pre>
  Modeline "640x480" 25.175  640 664  760  800  480 491 493 525
  Modeline "800x600" 36      800 824  896 1024  600 601 603 625
  ModeLine "832x624" 40      832 873 1001 1090  624 625 627 651
  Modeline "640x400" 25.175  640 664  760  800  400 409 411 450
</pre>
</p>



 <HR NOSHADE>
<A HREF="epson.html"><EM> Information for EPSON SPC8110 Users</EM></A>
 <b>:</b> <EM>Video modes </EM><BR>
<b>Previous:</b> <A HREF="epson2.html"><EM><code>XF86Config</code> options </EM></A><BR>
<b>Next:</b> <A HREF="epson4.html"><EM>Acknowledgments </EM></A>



</BODY>
</HTML>
