<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Acknowledgments </TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="tseng.html"><EM> Information for Tseng Chipset Users</EM></A>
 <b>:</b> <EM>Acknowledgments </EM><BR>
<b>Previous:</b> <A HREF="tseng15.html"><EM>Trouble shooting with the SVGA Tseng driver</EM></A><BR>
<b>Next:</b> <A HREF="tseng.html"><EM> Information for Tseng Chipset Users</EM></A>


<HR NOSHADE>
  <H2><A NAME="23"></A>16. Acknowledgments </H2>
<p>Most of these stem from the old XF86_W32 server. That code was used
extensively for getting the SVGA server to work on all the Tseng cards, so
they are still somewhat valid.</p>
<p>Glenn G. Lai wrote the original XF86_W32 server. It was modified by
Dirk Hohndel and Koen Gadeyne to support some more hardware.</p>
<p>Jerry J. Shekhel (<i>jerry@msi.com</i>) gave me (GGL) the 1-M Mirage
ET4000/W32 VLB board on which the initial development (X_W32) was done.</p>
<p>X11R6 and The XFree86 Project provide the base code for XF86_W32.</p>
<p>Hercules Computer Technology Inc. lent me (GGL) a 2-M Hercules Dynamite Pro VLB
board for the development that led to <code>XF86_W32</code>.   They donated a
Dynamite Power PCI to The XFree86 Project, that was used by DHH to extend
the server.</p>
<p>Tseng Labs kindly donated (KMG) an ET6000-based board (a Jazz Multimedia
G-Force 128), which spurred the development of the ET6000 code. They also
provided an ET6100 evaluation board.</p>
<p>Heiko Eissfeldt provided an ET4000W32p_rev_b board which allowed us to get
better support for those rev_a and rev_b boards.</p>
<p>Gyorgy Krajcsovits donated an ET4000W32p + CH8398 board. A Really Good Move!</p>
<p>Numerous testers have given me feedback for <code>X_W32</code> and later
<code>XF86_W32</code>.  I
apologize for my failure to keep track of the people who tested
<code>X_W32</code>, but
the names of the people involved with the <code>XF86_W32</code> testing are
listed below:
<dl>
<dt><b>Linux:</b><dd><p><i>bf11620@coewl.cen.uiuc.edu</i> (Byron Thomas Faber) <br>
<i>dlj0@chern.math.lehigh.edu</i> (David Johnson) <br>
<i>peterc@a3.ph.man.ac.uk</i> (Peter Chang)  <br>
<i>dmm0t@rincewind.mech.virginia.edu</i> (David Meyer) <br>
<i>nrh@philabs.Philips.COM</i> (Nikolaus R. Haus) <br>
<i>jdooley@dbp.caltech.edu</i> (James Dooley) <br>
<i>thumper@hitchcock.eng.uiowa.edu</i> (Timothy Paul Schlie) <br>
<i>klatta@pkdla5.syntex.com</i> (Ken Latta) <br>
<i>robinson@cnj.digex.net</i> (Andrew Robinson) <br>
<i>reggie@phys.washington.edu</i> (Reginald S. Perry) <br>
<i>sjm@cs.tut.fi</i> (M{kinen Sami J) <br>
<i>engel@yacc.central.de</i> (C. Engelmann) <b>use</b>
<i>cengelm@gwdg.de</i> <br>
<i>postgate@cafe.net</i> (Richard Postgate) <br>
<i>are1@cec.wustl.edu</i> (Andy Ellsworth) <br>
<i>bill@celtech.com</i> (Bill Foster)</p>
<dt><b> FreeBSD: </b><dd><p><i>ljo@ljo-slip.DIALIN.CWRU.Edu</i> (L Jonas Olsson)</p>
</dl>
</p>
<p>Several people have developed code for the SVGA Tseng driver (this list is
incomplete):
<ul>
<li>Glenn G. Lai</li>
<li>Dirk H. Hohndel</li>
<li>Koen Gadeyne</li>
<li>OEyvind Aabling</li>
<li>Dejan Ilic</li>
<li>Mark Vojkovich</li>
<li>Harald Nordgard Hansen</li>
<li>David Bateman</li>
<li>Gyorgy Krajcsovits</li>
<li>Kurt Olsen</li>
</ul>
</p>




<p>
<pre>
$XFree86: xc/programs/Xserver/hw/xfree86/doc/sgml/tseng.sgml,v 3.15.2.18 1998/11/13 13:00:48 dawes Exp $ 





$XConsortium: tseng.sgml /main/6 1996/10/27 11:06:09 kaleb $
</pre>
</p>

 <HR NOSHADE>
<A HREF="tseng.html"><EM> Information for Tseng Chipset Users</EM></A>
 <b>:</b> <EM>Acknowledgments </EM><BR>
<b>Previous:</b> <A HREF="tseng15.html"><EM>Trouble shooting with the SVGA Tseng driver</EM></A><BR>
<b>Next:</b> <A HREF="tseng.html"><EM> Information for Tseng Chipset Users</EM></A>



</BODY>
</HTML>
