<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Known problems in current driver</TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="rendition.html"><EM>Information for Rendition Users</EM></A>
 <b>:</b> <EM>Known problems in current driver</EM><BR>
<b>Previous:</b> <A HREF="rendition6.html"><EM>Major fixes in this release </EM></A><BR>
<b>Next:</b> <A HREF="rendition8.html"><EM>Work in progress (not finished in time for release) </EM></A>


<HR NOSHADE>
  <H2><A NAME="7"></A>7. Known problems in current driver</H2>
<p>
<ul>
<li>Displays with depth 15 ("-bpp 15" or "-bpp 16 -weight 555") has problems on V2x00 cards.</li>
<li>Switching from display to VC and back to display can lock up V2x00 cards.</li>
<li>When scrolling the virtual display on a V1000 card parts of the screen will become distorted. Problem dissapears when you continue moving around. V2x00 does not exhibit this problem. Probably a bug in the driver rather than a limitation of the chip.</li>
<li>Option "chipset" is honored. Unfortunatly the driver still has problems and will only work if the rendition card is the primary display card in the system.</li>
<li>Switching to VC does not restore correct textmode. Instead it defaults to 80x25.</li>
<li>A horizontal distortion around the hardware cursor can be seen on certain modes. It can be fixed by turning off hardware cursor or by lowering the required bandwith of the mode.</li>
</ul>
</p>

 <HR NOSHADE>
<A HREF="rendition.html"><EM>Information for Rendition Users</EM></A>
 <b>:</b> <EM>Known problems in current driver</EM><BR>
<b>Previous:</b> <A HREF="rendition6.html"><EM>Major fixes in this release </EM></A><BR>
<b>Next:</b> <A HREF="rendition8.html"><EM>Work in progress (not finished in time for release) </EM></A>



</BODY>
</HTML>
