<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Supported video-card chip-sets</TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="README.html"><EM>README for XFree86[tm] 3.3.5</EM></A>
 <b>:</b> <EM>Supported video-card chip-sets</EM><BR>
<b>Previous:</b> <A HREF="README2.html"><EM>Systems XFree86 has been tested on</EM></A><BR>
<b>Next:</b> <A HREF="README4.html"><EM>Where to get more information</EM></A>


<HR NOSHADE>
  <H2><A NAME="3"></A>3. Supported video-card chip-sets</H2>

<p>At this time, XFree86 3.3.5 supports the following chipsets:</p>
<p>
<dl>
<dt><b>Ark Logic</b><dd><p>ARK1000PV, ARK1000VL, ARK2000PV, ARK2000MT</p>
<dt><b>Alliance</b><dd><p>AP6422, AT24</p>
<dt><b>ATI </b><dd><p>18800, 18800-1, 28800-2, 28800-4, 28800-5, 28800-6, 68800-3, 68800-6,
68800AX, 68800LX, 88800GX-C, 88800GX-D, 88800GX-E, 88800GX-F, 88800CX,
264CT, 264ET, 264VT, 264GT, 264VT-B, 264VT3, 264GT-B, 264GT3
(this list includes the Mach8, Mach32, Mach64, 3D Rage, 3D Rage II and
3D Rage Pro)</p>
<dt><b>Avance Logic </b><dd><p>ALG2101, ALG2228, ALG2301, ALG2302, ALG2308, ALG2401</p>
<dt><b>Chips &amp; Technologies </b><dd><p>65520, 65525, 65530, 65535, 65540, 65545, 65546, 65548, 65550,
65554, 65555, 68554, 69000, 64200, 64300</p>
<dt><b>Cirrus Logic </b><dd><p>CLGD5420, CLGD5422, CLGD5424, CLGD5426, CLGD5428,
CLGD5429, CLGD5430, CLGD5434, CLGD5436, CLGD5440, CLGD5446, CLGD5462,
CLGD5464, CLGD5465, CLGD5480, CLGD6205, CLGD6215,
CLGD6225, CLGD6235, CLGD6410, CLGD6412, CLGD6420,
CLGD6440, CLGD7541(*), CLGD7543(*), CLGD7548(*), CLGD7555(*)</p>
<dt><b>Cyrix</b><dd><p>MediaGX, MediaGXm</p>
<dt><b>Compaq </b><dd><p>AVGA </p>
<dt><b>Digital Equipment Corporation </b><dd><p>TGA</p>
<dt><b>Epson</b><dd><p>SPC8110</p>
<dt><b>Genoa </b><dd><p>GVGA </p>
<dt><b>IBM </b><dd><p>8514/A (and true clones), XGA-2</p>
<dt><b>Intel </b><dd><p>i740</p>
<dt><b>IIT </b><dd><p>AGX-014, AGX-015, AGX-016</p>
<dt><b>Matrox</b><dd><p>MGA2064W (Millennium), MGA1064SG (Mystique and Mystique 220),
MGA2164W (Millennium II PCI and AGP), G100, G200, G400</p>
<dt><b>MX </b><dd><p>MX68000(*), MX680010(*)</p>
<dt><b>NCR </b><dd><p>77C22(*), 77C22E(*), 77C22E+(*)</p>
<dt><b>NeoMagic</b><dd><p>2200, 2160, 2097, 2093, 2090, 2070</p>
<dt><b>Number Nine</b><dd><p>I128 (series I, II and IV), Revolution 3D (T2R)</p>
<dt><b>NVidia/SGS Thomson </b><dd><p>NV1, STG2000, RIVA128, Riva TNT, Riva TNT2</p>
<dt><b>OAK </b><dd><p>OTI067, OTI077, OTI087</p>
<dt><b>RealTek</b><dd><p>RTG3106(*)</p>
<dt><b>Rendition</b><dd><p>V1000, V2x00</p>
<dt><b>S3 </b><dd><p>86C911, 86C924, 86C801, 86C805, 86C805i, 86C928, 86C864, 86C964,
86C732, 86C764, 86C765, 86C767, 86C775, 86C785, 86C868, 86C968,
86C325, 86C357, 86C362, 86C375, 86C375, 86C385, 86C988, 86CM65, 
86C260</p>
<dt><b>SiS</b><dd><p>86C201, 86C202, 86C205, 86C215, 86C225, 5597, 5598, 6326, 530, 620</p>
<dt><b>3dfx </b><dd><p>Voodoo Banshee, Voodoo3</p>
<dt><b>3DLabs </b><dd><p>GLINT 500TX, GLINT MX, Permedia, Permedia 2, Permedia 2v</p>
<dt><b>Tseng </b><dd><p>ET3000, ET4000AX, ET4000/W32, ET4000/W32i, ET4000/W32p, ET6000, ET6100</p>
<dt><b>Trident </b><dd><p>TVGA8800CS, TVGA8900B, TVGA8900C, TVGA8900CL, TVGA9000,
TVGA9000i, TVGA9100B, TVGA9200CXR, Cyber9320(*), TVGA9400CXi,
TVGA9420, TGUI9420DGi, TGUI9430DGi, TGUI9440AGi, TGUI9660XGi,
TGUI9680, ProVidia 9682, ProVidia 9685(*), Cyber 9382,
Cyber 9385, Cyber 9388, 3DImage975, 3DImage985, Cyber 9397,
Cyber 9520, Cyber 9525, Blade3D, CyberBlade</p>
<dt><b>Video 7/Headland Technologies </b><dd><p>HT216-32(*)</p>
<dt><b>Weitek </b><dd><p>P9000, P9100</p>
<dt><b>Western Digital/Paradise </b><dd><p>PVGA1 </p>
<dt><b>Western Digital </b><dd><p>WD90C00, WD90C10, WD90C11, WD90C24, WD90C24A, WD90C30, WD90C31,
WD90C33</p>
</dl>
</p>
<p>(*) Note, chips marked in this way have either limited support or
the drivers for them are not actively maintained.</p>
<p>All of the above are supported in both 256 color, and some are supported
in mono and 16 color modes, and some are supported an higher color depths.</p>
<p>Refer to the chipset-specific <code>README</code> files (currently for
<A href="DECtga.html">TGA</A>, <A href="MGA.html">Matrox</A>,
<A href="Mach32.html">Mach32</A>, <A href="Mach64.html">Mach64</A>,
<A href="NVIDIA.html">NVidia</A>, <A href="Oak.html">Oak</A>,
<A href="P9000.html">P9000</A>,
<A href="S3.html">S3 (except ViRGE)</A>,
<A href="S3V.html">S3 ViRGE</A>, <A href="SiS.html">SiS</A>,
<A href="Video7.html">Video7</A>,
<A href="WstDig.html">Western Digital</A>,
<A href="W32.html">Tseng (W32)</A>,
<A href="tseng.html">Tseng (all)</A>,
<A href="agx.html">AGX/XGA</A>, <A href="ark.html">ARK</A>,
<A href="ati.html">ATI (SVGA server)</A>,
<A href="chips.html">Chips and Technologies</A>,
<A href="cirrus.html">Cirrus</A>,
<A href="trident.html">Trident</A>,
<A href="neo.html">NeoMagic</A>,
<A href="rendition.html">Rendition</A>,
<A href="epson.html">Epson</A>,
<A href="3DLabs.html">3DLabs</A>)
<A href="i740.html">i740</A>)
for more information about using those chipsets.</p>
<p>The monochrome server also supports generic VGA cards, using 64k of video
memory in a single bank,
the Hercules monochrome card,
the Hyundai HGC1280,
Sigma LaserView, Visa and Apollo monochrome cards.</p>
<p>The VGA16 server supports memory banking with the ET4000, Trident, ATI,
NCR, OAK and Cirrus 6420 chipsets allowing virtual display sizes up to
about 1600x1200 (with 1MB of video memory).  For other chipsets the display
size is limited to approximately 800x600.</p>

 <HR NOSHADE>
<A HREF="README.html"><EM>README for XFree86[tm] 3.3.5</EM></A>
 <b>:</b> <EM>Supported video-card chip-sets</EM><BR>
<b>Previous:</b> <A HREF="README2.html"><EM>Systems XFree86 has been tested on</EM></A><BR>
<b>Next:</b> <A HREF="README4.html"><EM>Where to get more information</EM></A>



</BODY>
</HTML>
