<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Tested configurations. </TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="ark.html"><EM> Information for ARK Logic Chipset Users</EM></A>
 <b>:</b> <EM>Tested configurations. </EM><BR>
<b>Previous:</b> <A HREF="ark5.html"><EM>Features that may be expected in upcoming beta releases </EM></A><BR>
<b>Next:</b> <A HREF="ark.html"><EM> Information for ARK Logic Chipset Users</EM></A>


<HR NOSHADE>
  <H2><A NAME="6"></A>6. Tested configurations. </H2>

<p>
<dl>
<dt><b>Hercules Stringray Pro (ARK1000PV + ATT20C490-compatible RAMDAC)</b><dd><p>Supported at 8bpp, 16bpp and 24bpp. Fixed set of clocks.
There seems to be a restriction to the mode timings at 24bpp;
the last horizontal number (HTotal) must be divisible by 4 but
not by 8. If the modeline is wrong, the colors would
be incorrect. The driver automatically corrects the mode timing.</p>

<dt><b>Hercules Stingray Pro/V (ARK1000PV + IC Works ZoomDAC)</b><dd><p>Supported at 8bpp, 16bpp and 24bpp. Fixed set of clocks.
The same restrictions above exist for the 24bpp mode. Problems
with textmode restoration have been reported on some OS's.</p>

<dt><b>Hercules Stingray 64/V (ARK2000PV + IC Works ZoomDAC)</b><dd><p>Supported at 8bpp, 16bpp and 32bpp. Fixed set of clocks.
Problems with textmode restoration have been reported on
some OS's.</p>

<dt><b>Hercules Stingray 64 with ARK2000MT + ICS5342 Clockchip/RAMDAC</b><dd><p>This may also apply to other cards with the ICS5342, such as
the Diamond Stealth 64 Graphics 2001. Use RAMDAC "ics5342".
Programmable clockchip (don't specify any Clocks lines).
Supported at 8bpp, 16bpp and 32bpp. 32bpp has been reported not
to work. This configuration has not been tested with a post-3.2
server.</p>

</dl>
</p>
<p>If are having driver-related problems that are not addressed by this document,
you can try contacting the XFree86 team (the current driver maintainer
can be reached at <A href="mailto:H.Hanemaayer@inter.nl.net">H.Hanemaayer@inter.nl.net</A>), or post in the Usenet
newsgroup <A href="news:comp.windows.x.i386unix">comp.windows.x.i386unix</A>.</p>
<p>In fact, reports (success or failure) are very welcome, especially
on configurations that have not been tested. You can do this via the
<A href="http://www.xfree86.org/cgi-bin/bugform.cgi">bug report form</A>
(or send mail to <A href="mailto:XFree86@XFree86.org">XFree86@XFree86.org</A>). You may want to
keep an eye on forthcoming beta releases at the <A href="http://www.xfree86.org">XFree86 web site</A>.</p>

<p>
<pre>
$XFree86: xc/programs/Xserver/hw/xfree86/doc/sgml/ark.sgml,v 3.9 1997/01/25 03:22:20 dawes Exp $





$XConsortium: ark.sgml /main/6 1996/10/28 05:24:04 kaleb $
</pre>
</p>

 <HR NOSHADE>
<A HREF="ark.html"><EM> Information for ARK Logic Chipset Users</EM></A>
 <b>:</b> <EM>Tested configurations. </EM><BR>
<b>Previous:</b> <A HREF="ark5.html"><EM>Features that may be expected in upcoming beta releases </EM></A><BR>
<b>Next:</b> <A HREF="ark.html"><EM> Information for ARK Logic Chipset Users</EM></A>



</BODY>
</HTML>
