<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE> Information for Tseng Chipset Users</TITLE>
</HEAD>
<H1> Information for Tseng Chipset Users</H1>
<DL>
<DD>1. <A HREF="tseng1.html#1">Supported chipsets </A>
<DD>2. <A HREF="tseng2.html#2">Terminology </A>
<DD>3. <A HREF="tseng3.html#3">ET4000 driver features </A>
<DD>4. <A HREF="tseng4.html#4">ET6000 driver features </A>
<DD>5. <A HREF="tseng5.html#5">Clock selection problems with some ET4000 boards </A>
<DD>6. <A HREF="tseng6.html#6">Text mode restore problems </A>
<DD>7. <A HREF="tseng7.html#7">Basic configuration </A>
<DD>8. <A HREF="tseng8.html#8">general options in the <code>XF86Config</code> file </A>
<DD>9. <A HREF="tseng9.html#9">linear memory base address (MemBase) issues </A>
<DL>
<DD>9.1. <A HREF="tseng9.html#10">What you should know BEFORE trying another MemBase</A>
<DD>9.2. <A HREF="tseng9.html#11">Choosing a MemBase</A>
<DD>9.3. <A HREF="tseng9.html#12">An alternative approach</A>
<DD>9.4. <A HREF="tseng9.html#13">When all else fails...</A>
<DD>9.5. <A HREF="tseng9.html#14">Restrictions</A>
<DD>9.6. <A HREF="tseng9.html#15">Some boards simply cannot work in linear mode</A>
<DD>9.7. <A HREF="tseng9.html#16">How can I see if the linear address is wrong?</A>
</DL>
</DD>
<DD>10. <A HREF="tseng10.html#17">Mode issues </A>
<DD>11. <A HREF="tseng11.html#18">Acceleration issues </A>
<DD>12. <A HREF="tseng12.html#19">ET6000 memory size facts and fiction </A>
<DD>13. <A HREF="tseng13.html#20">ET6000 memory bandwidth hype and the impact on video modes </A>
<DD>14. <A HREF="tseng14.html#21">Linear addressing and 16bpp/24bpp/32bpp modes </A>
<DD>15. <A HREF="tseng15.html#22">Trouble shooting with the SVGA Tseng driver</A>
<DD>16. <A HREF="tseng16.html#23">Acknowledgments </A>
</DL>
</HTML>
