                        README for XFree86 on NetBSD

Rich  Murphey, David Dawes, Marc  Wandschneider, Mark  Weaver, Matthieu Herrb

                      Last modified on: 20 August 1999

1.  What and Where is XFree86?

XFree86 is a port of X11R6.3 that supports several versions of Intel-based
Unix.  It is derived from X386 1.2, which was the X server distributed with
X11R5.  This release consists of many new features and performance improve-
ments as well as many bug fixes.  The release is available as source patches
against the X Consortium X11R6.3 code, as well as binary distributions for
many architectures.

See the Copyright Notice.

The sources for XFree86 are available by anonymous ftp from:

ftp://ftp.XFree86.org/pub/XFree86/current

Binaries for NetBSD 1.4 and later are available from:
ftp://ftp.XFree86.org/pub/XFree86/current/binaries/NetBSD-1.4

A list of mirror sites is provided by ftp://ftp.XFree86.org/pub/XFree86/MIR-
RORS

Other NetBSD versions:

These binaries are not compatible with earlier NetBSD versions. If you're
still running NetBSD earlier than 1.4, you should think about upgrading to a
newer version of NetBSD first.

If you don't upgrade, you'll have to build XFree86 from the sources.  XFree86
should compile cleanly under earlier versions of NetBSD, although this has
not been tested.

XFree86 also builds on NetBSD/sparc. See section Building on other architec-
tures (section 9.5, page 1) for details.

The client side of XFree86 also builds on NetBSD/alpha and many other archi-
tecture supported by NetBSD.

XFree86 also supports NetBSD on PC98 machines.

2.  Bug Reports for This Document

Send email to matthieu@laas.fr (Matthieu Herrb) or XFree86@XFree86.org if you
have comments or suggestions about this file and we'll revise it.

3.  New OS-dependant features in XFree86 3.3.5

None.

See the Release Notes for non-OS dependent new features in XFree86 3.3.5.

4.  New OS-dependant features in XFree86 3.3.4

   o The maximum number of open connections in the server has been raised to
     128,

   o support for the wsmouse mouse protocol included in  NetBSD 1.4 has been
     added.

5.  Installing the Binaries

Refer to section 5 of the Release Notes  for detailed installation instruc-
tions.

6.  Configuring X for Your Hardware

The /etc/XF86Config file tells the X server what kind of monitor, video card
and mouse you have.  You must create it to tell the server what specific
hardware you have.

The easiest way to create this file is to run the XF86Setup utility as root.
Refer to QuickStart.doc for details about its use.

You'll need info on your hardware:

   o Your mouse type, baud rate and its /dev entry.

   o The video card's chipset (e.g. ET4000, S3, etc).

   o Your monitor's sync frequencies.

The recommended way to generate an XF86Config file is to use the XF86Setup
utility.  The xf86config text utility is still there for the (few) cases
where XF86Setup can't be used. Also, there is a sample file installed as
/usr/X11R6/lib/X11/XF86Config.eg, which can be used as a starting point.

For details about the XF86Config file format, refer to the XF86Config(5) man-
ual page.

Once you've set up a XF86Config file, you can fine tune the video modes with
the xvidtune utility.

6.1  About mouse configuration

If your serial mouse does not work try using kermit or tip to connect to the
mouse serial port and verify that it does indeed generate characters.

The NetBSD pms mouse driver handles PS/2 style mice as Busmouse. Specify the
protocol as ``busmouse'' in the mouse section of your XF86Config file if
you're using a PS/2 mouse.

Only standard PS/2 mice are supported by this driver. Newest PS/2 mice that
send more than three bytes at a time (especially Intellimouse, or MouseMan+
with a ``3D'' roller) are not supported yet.

XFree86 3.3.4 and later also have support for the mouse driver included in
the new wscons console driver introduced by NetBSD 1.4. Specify ``wsmouse''
as the protocol and ``/dev/wsmouse0'' as the device in /etc/XF86Config if
you're using NetBSD 1.4 with wscons.

See README.mouse  for general instruction on mouse configuration in XFree86.

6.2  Other input devices

XFree86  supports the dynamic loading of drivers for external input devices
using the XInput extension. Currently supported devices are:

   o Joystick (xf86Jstk.so)

   o Wacom tablets (Wacom IV protocol only, xf86Wacom.so)

   o SummaSketch tablets (xf86Summa.so)

   o Elographics touchscreen (xf86Elo.so)

To use a specific device, add the line

     load "module"

in the Module section of XF86Config, where module is the name of the .so file
corresponding to your device.  You also need to set up a XInput section in
XF86Config.  Refer to the XF86Config(5) man page for detailed configuration
instructions.

You can then change the device used to drive the X pointer with the xset-
pointer(1) command.

For joystick support, you'll need to install the joystick device driver in
the kernel. It is included in NetBSD 1.2. See joy(4) for details.

6.3  Configuring PEX and XIE extensions

The PEX and XIE extensions are  supported as external modules.  If you want
to have access to these extensions, add the following lines to the Module
section of XF86Config:

        load    "pex5.so"
        load    "xie.so"

7.  Running X

8mb of memory is a recommended minimum for running X.  The server, window
manager and an xterm take about 4 Mb of memory themselves.  On a 4Mb system
that would leave nothing left over for other applications like gcc that
expect a few meg free.  X will work with 4Mb of memory, but in practice com-
pilation while running X can take 5 or 10 times as long due to constant pag-
ing.

The easiest way for new users to start X windows is to type:

     startx >& startx.log

Error messages are lost unless you redirect them because the server takes
over the screen.

To get out of X windows, type: ``exit'' in the console xterm.  You can cus-
tomize your X by creating .xinitrc, .xserverrc, and .twmrc files in your home
directory as described in the xinit and startx man pages.

7.1  Starting Xdm, the display manager

To start the display manager, log in as root on the console and type: ``xdm
-nodaemon''.

You can start xdm automatically on bootup by disabling the console getty and
adding the following code to /etc/rc.local:

       if [ -x /usr/X11R6/bin/xdm ]; then
         echo -n ' xdm'; /usr/X11R6/bin/xdm
       fi

To disable the console getty, change ``on'' to ``off'' in the console entry
in /etc/ttys:

      ttyv0    "/usr/libexec/getty Pc"  pc   off secure

Under NetBSD 1.4 with the wscons console driver, you must enable a virtual
console for the X server first. To do this follow these steps:

   o Make sure the device file exists. If not, ``cd /dev ; ./MAKEDEV
     wscons''.

   o Next, make sure your kernel wants to do wscons. (see below (section 8.1,
     page 1)).

   o Next, make sure ``wscons=YES'' in /etc/rc.conf.

   o Next, make sure /etc/wscons.conf exists. The relevant bits:

          #screen   0    -    vt100
          screen    1    -    vt100
          screen    2    -    vt100
          screen    3    -    vt100
          screen    4    -    -
          screen    5    -    vt100

(Thanks to Mason Loring Bliss <mason@acheron.middleboro.ma.us> for this
explanation)

Note that the binary distributions of XFree86 for NetBSD don't include sup-
port for the XDM-AUTHORIZATION-1 protocol.

8.  Kernel Support for X

To make sure X support is enabled under NetBSD, the following line must be in
your config file in /sys/arch/i386/conf:

     options XSERVER, UCONSOLE

8.1  Console drivers

The server supports the standard NetBSD/i386 console drivers: pccons, pcvt
and wscons (in pcvt compatibility mode). They are detected at runtime and no
configuration of the server itself is required.

The pccons driver is the most widely tested and is the console driver con-
tained in the NetBSD binary distribution's kernels.

The pcvt console driver is bundled with NetBSD. The pcvt X mode is compatible
with the pccons driver X mode. It offers several virtual consoles and inter-
national keyboard support. In order to use this driver, change the line:

     device          pc0     at isa? port "IO_KBD" irq 1

to

     device         vt0     at isa? port "IO_KBD" irq 1

in your kernel config file, and rebuild and install your kernel.

XFree86 will also run with the wscons console driver in NetBSD 1.4. For now,
it uses the pcvt compatibility mode, so be sure to have the lines:

     options         WSDISPLAY_COMPAT_PCVT           # emulate some ioctls
     options         WSDISPLAY_COMPAT_SYSCONS        # emulate some ioctls
     options         WSDISPLAY_COMPAT_USL         # VT handling
     options         WSDISPLAY_COMPAT_RAWKBD         # can get raw scancodes

in your kernel configuration file if you're using wscons. Refer to the
wscons(4) and wsmouse(4) manual pages for informations on how to configure
wscons into the kernel.

8.2  Aperture Driver

By default NetBSD 0.9C and higher include the BSD 4.4 kernel security feature
that disable access to the /dev/mem device when in multi-users mode. But
XFree86 servers can take advantage (or require) linear access to the display
memory.

Moset recent accelerated servers require linear memory access, some other can
take advantage of it, but do not require it.

There are two ways to allow XFree86 to access linear memory:

The first way is to disable the kernel security feature by adding `option
INSECURE' in the kernel configuration file and build a new kernel.

The second way is to install the aperture driver: You can get the aperture
driver sources from ftp://ftp.netbsd.org/pub/NetBSD/arch/i386/apNetBSD.shar.

How to activate it is highly dependent from your exact operating system ver-
sion:

   o  NetBSD 1.0, 1.1, 1.2, 1.2.1:

     Add the following lines to the end of /etc/rc.local:

           KERNDIR=/usr/X11R6/lib/X11/kernel
           if [ -f ${KERNDIR}/ap.o ]; then
             modload -o ${KERNDIR}/ap -e ap -p ${KERNDIR}/apinstall ${KERNDIR}/ap.o
           fi

   o  NetBSD 1.2D and later

     Add the following line to  /etc/lkm.conf:

          /usr/X11R6/lib/X11/kernel/ap.o  -  ap /usr/X11R6/lib/X11/kernel/apinstall -

   o  NetBSD 1.2G, 1.3 and later

     The lkm.conf format changed in 1.2G.  Add the following line to
     /etc/lkm.conf:

          /usr/X11R6/lib/X11/kernel/ap.o  -  ap /usr/X11R6/lib/X11/kernel/apinstall - -AFTERMOUNT

Reboot your system. XFree86 will auto-detect the aperture driver if avail-
able.

Warning: if you boot another kernel than /netbsd or /bsd, loadable kernel
modules can crash your system. Always boot in single user mode when you want
to run another kernel.

     Caveat: the  aperture driver only allows one access at a time (so
     that the system is in the same security state once X is launched).
     This means that if you run multiple servers on multiples VT, only
     the first one will have linear memory access.  Use 'option INSE-
     CURE' if you need more that one X server at a time.

8.3  MIT-SHM

NetBSD 1.0 and later supports System V shared memory. If XFree86 detects this
support in your kernel, it will support the MIT-SHM extension.

To add support for system V shared memory to your kernel add the lines:

      # System V-like IPC
      options         SYSVMSG
      options         SYSVSEM
      options         SYSVSHM

to your kernel config file.

9.  Rebuilding the XFree86 Distribution

The server link kit allow you to rebuild just the X server with a minimum
amount of disk space.  Just unpack it, make the appropriate changes to the
xf86site.def, type ``./mkmf'' and ``make'' to link the server.  See
/usr/X11R6/lib/Server/README for more info.

See INSTALL for instructions on unbundling and building the source distribu-
tion.

You should configure the distribution by editing xc/config/cf/host.def
before compiling.  To compile the sources, invoke ``make World'' in the xc
directory.

9.1  Console drivers

XFree86 has a configuration option to select the console drivers to use in
xf86site.def:

   o  if you're using pccons put:

           #define XFree86ConsoleDefines -DPCCONS_SUPPORT

   o if you're using pcvt put:

           #define XFree86ConsoleDefines -DPCVT_SUPPORT

   o if you're using syscons put:

           #define XFree86ConsoleDefines -DSYSCONS_SUPPORT

   o if you're running codrv put:

           #define XFree86ConsoleDefines -DCODRV_SUPPORT

If you don't define XFree86ConsoleDefines in xf86site.def the pccons and pcvt
drivers will be supported by default.

Syscons and codrv are not bundled with NetBSD. They are available by anony-
mous FTP from a number of sites. They are not supported by the XFree86 binary
distribution anymore.

9.2  pcvt_ioctl.h file:

XFree86's default configuration includes support for the PCVT console driver.
Unfortunately, NetBSD versions before 19980413 don't install the pcvt_ioctl.h
file in /usr/include/machine. If you want to build XFree86 with PCVT support,
execute the following command as root before starting make World:

     cp /usr/src/sys/arch/i386/isa/pcvt/pcvt_ioctl.h /usr/include/machine

If you don't have kernel sources, you can grab this file from ftp.netbsd.org
or one of its mirrors. If you're not running PCVT, you can remove -DPCVT_SUP-
PORT from XFree86ConsoleDefines in xf86site.def too.

9.3  console.h and ioctl_pc.h files:

If you want to build a server supporting codrv and you don't already have the
corresponding header file ioctl_pc.h installed in /usr/include/machine, then
install the copy that is supplied in xc/programs/Xserver/hw/xfree86/etc.  If
you run NetBSD-current you probably want to install it in
/usr/src/sys/arch/i386/include too, so that it get reinstalled each time you
run make includes.

If you have installed the  codrv console driver, this file should be taken
from your installed version of the driver.

The console.h file for syscons isn't distributed with XFree86 anymore. You
should get it from the syscons distribution.

9.4  Support for shared libs under NetBSD 1.0 and later

By default XFree86 builds for NetBSD with shared libraries support. If you're
building on 0.9 or don't want shared libraries add the following line to
host.def:

     #define BuildBsdSharedLibs    NO

9.5  Building on other architectures

XFree86 also compiles on NetBSD/sparc. The Sun server patches from Dennis
Ferguson and Matthew Green have been integrated in xc/pro-
grams/Xserver/hw/sun.  Small modifications to xf86site.def are needed:

   o Set all variables defining the servers to build to NO. (The variables
     controlling the Sun servers to build Xsun24Server, XsunServer and Xsun-
     MonoServer are defined at the end of NetBSD.cf.)

   o Set ServerToInstall to the sun server of your choice. (Xsun or Xsun-
     Mono).

   o Look at other applicable options in the INSTALL document.

Problems with this port should be reported to the port-sparc@NetBSD.Org mail-
ing list or directly to me matthieu@laas.fr rather than to the xfree86 mail-
ing list.

Note that the NetBSD project has now its own source tree, based on the
XFree86 source tree, with some local modifications. You may want to start
with this tree to rebuild from sources.  The NetBSD xsrc source tree is
available at: ftp://ftp.netbsd.org/pub/NetBSD/NetBSD-current/xsrc/

10.  Building New X Clients

The easiest way to build a new client (X application) is to use xmkmf if an
Imakefile is included in the sources.  Type ``xmkmf -a'' to create the Make-
files, check the configuration if necessary and type ``make''.  Whenever you
install additional man pages you should update whatis.db by running ``make-
whatis /usr/X11R6/man''.

To avoid the ``Virtual memory exhausted'' message from cc while compiling,
increase the data and stack size limits (in csh type ``limit datasize 32M''
and ``limit stacksize 16M'').

Note: Starting with XFree86 2.1 and NetBSD 0.9A, the symbol __386BSD__ no
longer gets defined either by the compiler or via the X config files for *BSD
systems.  When porting clients to *BSD systems, make use of the symbol BSD
for code which is truly BSD-specific.  The value of the symbol can be used to
distinguish different BSD releases.  For example, code specific to the Net-2
and later releases can use:

     #if (BSD >= 199103)

To ensure that this symbol is correctly defined, include <sys/param.h> in the
source that requires it.  Note that the symbol CSRG_BASED is defined for *BSD
systems in XFree86 3.1.1 and later.  This should be used to protect the
inclusion of <sys/param.h>.

For code that really is specific to a particular i386 BSD port, use
__FreeBSD__ for FreeBSD, __NetBSD__ for NetBSD, __OpenBSD__ for OpenBSD,
__386BSD__ for 386BSD, and __bsdi__ for BSD/386.

Another note: If you get the message:

     ld.so: undefined symbol _XtCvtStringToFont

at run-time, you've stumbled on a semantic weakness of the NetBSD dynamic
linker. Applications that use libXmu also need libXt. If the client uses a
standard Imakefile, this dependency will probably by included in the Makefile
automagically -- you'll not see the problem. Otherwise, just add ``-lXt'' to
your library list in the Imakefile or Makefile and relink.

11.  Thanks

Many thanks to:

   o Pace Willison for providing the initial port to 386BSD.

   o Amancio Hasty for fixing cursor restoration, mouse bugs and many others.

   o Christoph Robitschko for fixing com.c and thus select().

   o Nate Williams for the patchkit support for X.

   o Rod Grimes and Jack Velte of Walnut Creek Cdrom for use of their
     machines in preparing the FreeBSD binary release.

     Generated from XFree86: xc/programs/Xserver/hw/xfree86/doc/sgml/NetBSD.sgml,v 3.45.2.13 1999/08/23 08:49:48 hohndel Exp $

     $XConsortium: NetBSD.sgml /main/26 1996/10/28 05:43:20 kaleb $

