<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>16bpp and 32bpp</TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="S3.html"><EM> Information for S3 Chipset Users</EM></A>
 <b>:</b> <EM>16bpp and 32bpp</EM><BR>
<b>Previous:</b> <A HREF="S31.html"><EM>Supported hardware</EM></A><BR>
<b>Next:</b> <A HREF="S33.html"><EM>List of Supported Clock Chips</EM></A>


<HR NOSHADE>
  <H2><A NAME="2"></A>2. 16bpp and 32bpp</H2>

<p>On 801/805 + AT&amp;T490 Cards (like the Fahrenheit 1280+ VLB) only 15 and
16bpp are supported. 32bpp isn't available on this type of
card. (There is a 24 bit mode under MS Windows, but it's not a 32bpp
sparse mode but a real 3 bytes/pixel mode).</p>

 <HR NOSHADE>
<A HREF="S3.html"><EM> Information for S3 Chipset Users</EM></A>
 <b>:</b> <EM>16bpp and 32bpp</EM><BR>
<b>Previous:</b> <A HREF="S31.html"><EM>Supported hardware</EM></A><BR>
<b>Next:</b> <A HREF="S33.html"><EM>List of Supported Clock Chips</EM></A>



</BODY>
</HTML>
