<!DOCTYPE HTML PUBLIC "-//IETF//DTD HTML Strict//EN">
<html><head><title>
Configuration Options
</title></head><body><h3>
Configuration Options
</h3><hr>

<p><h4>Basic Configuration Options - the <code>configure</code>
utility</h4>

<p>The following options are for compiling and installing a working
version of the xntp3 distribution. In most cases, the build process is
completely automatic. In some cases where memory space is at a premium,
or the binaries are to be installed in a different place, it is possible
to tailor the configuration to remove such features as reference clock
driver support, debugging support, and so forth.

<p>Configuration options are specified as arguments to the
<code>configure</code> script. Following is a summary of the current
options:
<p>
Usage: configure [options] [host]<br>
Options: [defaults in brackets after descriptions]

<p><pre>
Configuration

  --cache-file=FILE      cache test results in FILE
  --help                 print this message
  --no-create            do not create output files
  --quiet, --silent      do not print `checking...' messages
  --version              print the version of autoconf that created
                         configure
Directory and file names

  --prefix=PREFIX        install architecture-independent files in
                         PREFIX [/usr/local]
  --exec-prefix=EPREFIX  install architecture-dependent files in EPREFIX
                         [same as prefix]
  --bindir=DIR           user executables in DIR [EPREFIX/bin]
  --sbindir=DIR          system admin executables in DIR [EPREFIX/sbin]
  --libexecdir=DIR       program executables in DIR [EPREFIX/libexec]
  --datadir=DIR          read-only architecture-independent data in DIR
                         [PREFIX/share]
  --sysconfdir=DIR       read-only single-machine data in DIR
                         [PREFIX/etc]
  --sharedstatedir=DIR   modifiable architecture-independent data in DIR
                         [PREFIX/com]
  --localstatedir=DIR    modifiable single-machine data in DIR
                         [PREFIX/var]
  --libdir=DIR           object code libraries in DIR [EPREFIX/lib]
  --includedir=DIR       C header files in DIR [PREFIX/include]
  --oldincludedir=DIR    C header files for non-gcc in DIR
                         [/usr/include]
  --infodir=DIR          info documentation in DIR [PREFIX/info]
  --mandir=DIR           man documentation in DIR [PREFIX/man]
  --srcdir=DIR           find the sources in DIR [configure dir or ..]
  --program-prefix=PREFIX prepend PREFIX to installed program names
  --program-suffix=SUFFIX append SUFFIX to installed program names
  --program-transform-name=PROGRAM run sed PROGRAM on installed program
                         names
Host type

  --build=BUILD          configure for building on BUILD [BUILD=HOST]
  --host=HOST            configure for HOST [guessed]
  --target=TARGET        configure for TARGET [TARGET=HOST]
Features and packages

  --disable-FEATURE      do not include FEATURE (same as --enable-
                         FEATURE=no)
  --enable-FEATURE[=ARG] include FEATURE [ARG=yes]
  --with-PACKAGE[=ARG]   use PACKAGE [ARG=yes]
  --without-PACKAGE      do not use PACKAGE (same as --with-PACKAGE=no)
  --x-includes=DIR       X include files are in DIR
  --x-libraries=DIR      X library files are in DIR

--enable- and --disable- with options recognized

     debugging           Include debugging code [enable]
     gdt-surveying       Include GDT survey code [disable]
     md5                 Include support for MD5 keys [enable]
     des                 Include support for DES keys [enable]
     all-clocks          Include drivers for all reference clocks
                         [enable]

  Radio Clocks (these are ordinarily enabled, if supported by the
                         machine and operating system)

     ACTS                NIST dialup clock
     ARBITER             Arbiter 1088A/B GPS receiver
     AS2201              Austron 2200A or 2201A GPS receiver
     ATOM                ATOM clock
     BANCOMM             BANCOMM clock
     CHU                 CHU clock
     DATUM               Datum Programmable Time System
     DCF7000             ELV/DCF7000
     GPSVME              GPS-VME Clock
     HEATH               HeathKit GC-1000 Most Accurate Clock
     HOPF6021            HOPF6021 Radio Clock support
     HPGPS               HP 58503A GPS Time & Frequency receiver
     IRIG                IRIG (Audio) Clock
     LEITCH              Leitch CSD 5300 Master Clock System Driver
     LOCAL-CLOCK         Local Clock driver
     MEINBERG            Meinberg clocks
     MSFEES              MSFEES clock
     MOTO                Motorola GPS clock
     MX4200              MX4200 clock
     NMEA                NMEA GPS clock
     PARSE               PARSE clock code
     PST                 PST/Traconex 1020 WWV/H receiver
     PTBACTS             PTB dialup clock support
     RAWDCF              use raw DCF77 time code
     RCC8000             RCC8000 Radio Clock support
     SCHMID              SCHMID DCF77 clock support
     TRAK                TRAK 8810 GPS station clock
     TPRO                KSI/Odetics TPRO/S IRIG Interface
     TRIMTAIP            Trimble GPS/TAIP Protocol
     TRIMTSIP            Trimble GPS/TSIP Protocol
     TRUETIME            Kinemetrics/TrueTime (generic) receiver
     WWVB                Spectracom 8170 or Netclock/2 WWVB receiver
     USNO                US Naval Observatory dialup clock

  Miscellany

     accurate-adjtime    The adjtime() call is accurate
     kmem                Read kmem
     tick=VALUE          Force a value for 'tick'
     tickadj=VALUE       Force a value for 'tickadj'
     udp-wildcard        Use UDP wildcard delivery
     slew-always         Always slew the time
     step-slew           Step and slew the time
     ntpdate-step        If ntpdate should step the time
     hourly-todr-sync    If we should sync TODR hourly
</pre><p>

<hr><address>David L. Mills (mills@udel.edu)</address></body></html>
