/*
 *	linux/arch/alpha/kernel/sys_eiger.c
 *
 *	Copyright (C) 1995 David A Rusling
 *	Copyright (C) 1996, 1999 Jay A Estabrook
 *	Copyright (C) 1998, 1999 Richard Henderson
 *	Copyright (C) 1999 Iain Grant
 *
 * Code supporting the EIGER (EV6+TSUNAMI).
 */

#include <linux/kernel.h>
#include <linux/types.h>
#include <linux/mm.h>
#include <linux/sched.h>
#include <linux/pci.h>
#include <linux/init.h>

#include <asm/ptrace.h>
#include <asm/system.h>
#include <asm/dma.h>
#include <asm/irq.h>
#include <asm/bitops.h>
#include <asm/mmu_context.h>
#include <asm/io.h>
#include <asm/pci.h>
#include <asm/pgtable.h>
#include <asm/core_tsunami.h>
#include <asm/hwrpb.h>

#include "proto.h"
#include "irq.h"
#include "bios32.h"
#include "machvec.h"

#define dev2hose(d) (bus2hose[(d)->bus->number]->pci_hose_index)

/*
 * HACK ALERT! only the boot cpu is used for interrupts.
 */

static void
eiger_update_irq_hw(unsigned long irq, unsigned long unused, int unmask_p)
{

	unsigned int regaddr;
	unsigned long mask;

	if (irq <= 15) {
		if (irq <= 7)
			outb(alpha_irq_mask, 0x21);		/* ISA PIC1 */
	else
			outb(alpha_irq_mask >> 8, 0xA1);	/* ISA PIC2 */
	} else {
		if (irq > 63)
			mask = _alpha_irq_masks[1] << 16;
		else
			mask = _alpha_irq_masks[0] >> ((irq - 16) & 0x30);

		regaddr = 0x510 + (((irq - 16) >> 2) & 0x0c);

		outl(mask & 0xffff0000UL, regaddr);
	}

}

static void
eiger_device_interrupt(unsigned long vector, struct pt_regs * regs)
{
	unsigned intstatus;

	/*
	 * The PALcode will have passed us vectors 0x800 or 0x810,
	 * which are fairly arbitrary values and serve only to tell
	 * us whether an interrupt has come in on IRQ0 or IRQ1. If
	 * it's IRQ1 it's a PCI interrupt; if it's IRQ0, it's
	 * probably ISA, but PCI interrupts can come through IRQ0
	 * as well if the interrupt controller isn't in accelerated
	 * mode.
	 *
	 * OTOH, the accelerator thing doesn't seem to be working
	 * overly well, so what we'll do instead is try directly
	 * examining the Master Interrupt Register to see if it's a
	 * PCI interrupt, and if _not_ then we'll pass it on to the
	 * ISA handler.
	 */

	intstatus = inw(0x500) & 15;
	if (intstatus) {
		/*
		 * This is a PCI interrupt. Check each bit and
		 * despatch an interrupt if it's set.
		 */

		if (intstatus & 8) handle_irq(16+3, 16+3, regs);
		if (intstatus & 4) handle_irq(16+2, 16+2, regs);
		if (intstatus & 2) handle_irq(16+1, 16+1, regs);
		if (intstatus & 1) handle_irq(16+0, 16+0, regs);
	} else
		isa_device_interrupt (vector, regs);
}


static void
eiger_srm_device_interrupt(unsigned long vector, struct pt_regs * regs)
{
   int irq = (vector - 0x800) >> 4;

   handle_irq(irq, irq, regs);

}

static void __init
eiger_init_irq(void)
{
	outb(0, DMA1_RESET_REG);
	outb(0, DMA2_RESET_REG);
	outb(DMA_MODE_CASCADE, DMA2_MODE_REG);
	outb(0, DMA2_MASK_REG);

	if (alpha_using_srm)
		alpha_mv.device_interrupt = eiger_srm_device_interrupt;

	eiger_update_irq_hw(16, alpha_irq_mask, 0);

	enable_irq(2);
}

static int __init
eiger_map_irq(struct pci_dev *dev, int slot, int pin)
{
	u8 irq_orig;
	int irq;

	/* The SRM console has already calculated out the IRQ value's for
	   option cards. As this works lets just read in the value already
	   set and change it to a useable value by Linux.

	   All the IRQ values generated by the console are greater than 90,
	   so we calculate a value for Linux by the following:

	   irq = (card Irq - 80);

	   We subtract 80 because it is (90 - allocated ISA IRQ's ).
	*/
	pcibios_read_config_byte(dev->bus->number,
				 dev->devfn,
				 PCI_INTERRUPT_LINE,
				 &irq_orig);

	irq = ( irq_orig - 0x80);

	return irq;
}

/* New swizzle routine with code for card based bridges */
static int __init
eiger_swizzle(struct pci_dev *dev, int *pinp)
{
	int slot, pin = *pinp;
	int bridge_count = 0;

	/* Find the number of backplane bridges */
	int backplane = ( inw(0x502) & 0x0f);

	switch (backplane)
	{
	   case 0x00: bridge_count = 0; break; /* No bridges */
	   case 0x01: bridge_count = 1; break; /* 1 */
	   case 0x03: bridge_count = 2; break; /* 2 */
	   case 0x07: bridge_count = 3; break; /* 3 */
	   case 0x0f: bridge_count = 4; break; /* 4 */
	};


	/*  Check first for the built-in bridges on hose 0. */
	if ( dev2hose(dev) == 0 &&
            ( (PCI_SLOT(dev->bus->self->devfn) > (20-bridge_count))))
	{
		slot = PCI_SLOT(dev->devfn);
	} else {
		/*  Must be a card-based bridge.  */
		do {
			/* Check for built-in bridges on hose 0. */
			if ( dev2hose(dev) == 0 &&
			     (PCI_SLOT(dev->bus->self->devfn) >
				(20 - bridge_count)))
			{
                  		slot = PCI_SLOT(dev->devfn);
				break;
			}
			pin = bridge_swizzle(pin, PCI_SLOT(dev->devfn)) ;

			/* Move up the chain of bridges.  */
			dev = dev->bus->self;
			/* Slot of the next bridge.  */
			slot = PCI_SLOT(dev->devfn);
		} while (dev->bus->self);
	}
	*pinp = pin;

	return slot;
}

static void __init
eiger_pci_fixup(void)
{
	layout_all_busses(DEFAULT_IO_BASE, DEFAULT_MEM_BASE);
	common_pci_fixup(eiger_map_irq, eiger_swizzle);
}

/*
 * The System Vectors
 */

struct alpha_machine_vector eiger_mv __initmv = {
	vector_name:		"Eiger",
	DO_EV6_MMU,
	DO_DEFAULT_RTC,
	DO_TSUNAMI_IO,
	DO_TSUNAMI_BUS,
	machine_check:		tsunami_machine_check,
	max_dma_address:	ALPHA_MAX_DMA_ADDRESS,

	nr_irqs:		128,
	irq_probe_mask:		TSUNAMI_PROBE_MASK,
	update_irq_hw:		eiger_update_irq_hw,
	ack_irq:		generic_ack_irq,
	device_interrupt:	eiger_device_interrupt,

	init_arch:		tsunami_init_arch,
	init_irq:		eiger_init_irq,
	init_pit:		generic_init_pit,
	pci_fixup:		eiger_pci_fixup,
	kill_arch:		generic_kill_arch,
};
ALIAS_MV(eiger)
