! Copyright (c) 1990-1997  Michael Sandrof, Troy Rollo, Matthew Green,
! and other ircII contributors.
!
! All rights reserved.  See the HELP IRCII COPYRIGHT file for more
! information.
!
Usage: SET HOLD_MODE_MAX <number of lines>
  This specifies the maximum number of lines that will be held
  in HOLD_MODE before the display is automatically restarted.
  If HOLD_MODE_MAX is 0, the number of lines held in HOLD_MODE
  is unlimited.
