	ISA PnP utilities Version 1.18
	==============================

These programs allow ISA Plug-And-Play devices to be configured
on a Linux machine.

This program is suitable for all systems, whether or not they
include a PnP BIOS. In fact, a PnP BIOS adds some complications
because it may already activate some cards so that the drivers
can find them, and these tools can unconfigure them, or change
their settings causing all sorts of nasty effects. If you have
(for example) plug and play network cards that already work, I
suggest you read the manual page isapnp.conf(5) on the format
of the configuration file very carefully.

See the example for a dataflex voice fax modem and NE2000 clone
PnP card in README.modules. See the section below on Drivers and
MODULES for more background information. For even more hints etc
see the FAQ at:

 http://www.roestock.demon.co.uk/isapnptools/isapnpfaq.html

The commands have been taken from the Plug and Play ISA
specification Version 1.0a, widely available on the net.
(ftp://ftp.microsoft.com/developr/drg/Plug-and-Play/Pnpspecs/PNPISA.EXE -
this is a self-extracting DOS archive of PNPISA.DOC - a
word 6 document. If Word 6 not available, use the freely
redistributable viewer wordview which comes on the Win95 CD).

See CHANGES for a list of changes from the previous version.

See README.OS2 for description of OS2 stuff.

Installation intructions
========================
See the file INSTALL.

Format of pnp configuration file:
=================================
See the manual page isapnp.conf.5.

If you have a problem:
======================
Please start by looking at ALL the documentation provided, including
the FAQ, then look at the isapnptools website at
http://www.roestock.demon.co.uk/isapnptools/

Drivers and MODULES
===================
Note that boards first configured by isapnp are not visible to the kernel
during boot up. This means that drivers for the boards must be loaded
as modules after the board has been configured, so that they can
locate the board. See README.modules for an example.

This doesn't apply to serial cards, because setserial can be used to
configure the serial ports after the kernel has booted.

Also, IDE devices can be initialised after the kernel boots by
configuring IDE-PCMCIA in the kernel. Then writing a module to
initialise the device after running isapnp.
See README.ide and /usr/src/linux/Documentation/Configure.help.

An alternative method is to use initrd to run isapnp before booting
the main kernel. See README.initrd and /usr/src/linux/Documentation/initrd.txt.
This may be particularly applicable for IDE devices attached to PnP cards.
I hope to experiment with initrd sometime for my network card...
if you've already done it please tell me how.

If you boot Linux from DOS using loadlin, you can also run the DOS
version of isapnp before booting Linux. This would allow you to use
normal compiled in drivers.

If the kernel needs rebooting after configuration, because the drivers
are not modules, it may be possible to do this automatically in your
bootup scripts: use an isapnp.conf file which dumps the board
configuration registers and tests the the output.
If the board(s) haven't been configured, configure them with the
configuration isapnp.conf file and reboot.
If the boards have been configured, continue the boot normally.
You may want to take precautions to prevent the kernel continuously
rebooting if something goes wrong...

isapnp for debugging.
=====================
This example shows how the PEEK command may now be used with the standard
configuration settings to dump the actual board configuration register
settings, for example, the script:

#(DEBUG)
(READPORT 0x3bb)
#(READPORT 0x203)
(ISOLATE PRESERVE)
(IDENTIFY *)
(CONFIGURE DFX0000/1493
        (LD 0
                (IO 0 (PEEK)) # Dump Port 0
                (IO 1 (PEEK)) # Dump Port 1
                (IO 2 (PEEK)) # Dump Port 2
                (INT 0 (PEEK)) # Dump INT 0
                (DMA 0 (PEEK)) # Dump DMA 0
                (DMA 1 (PEEK)) # Dump DMA 1
                (MEM 0 (PEEK)) # Dump MEM 0
                (REG 0x60 (PEEK)) (REG 0x61 (PEEK)) # Dump Port 0
                (REG 0x62 (PEEK)) (REG 0x63 (PEEK)) # Dump Port 1
                (REG 0x64 (PEEK)) (REG 0x65 (PEEK)) # Dump Port 2
                (REG 0x70 (PEEK)) (REG 0x71 (PEEK)) # Dump INT 0
                (REG 0x74 (PEEK)) # Dump DMA 0
                (REG 0x75 (PEEK)) # Dump DMA 1
))
(WAITFORKEY)

produces the following with my dataflex modem:

Board 1 has Identity 6e 00 00 05 d5 00 00 d8 10:  DFX0000 Serial No 1493 [checksum 6e]
Peek(DFX0000/1493)[0][0x60](IO  0) is 0x03E8, (3,232)
Peek(DFX0000/1493)[0][0x62](IO  1) is 0x0000, (0,0)
Peek(DFX0000/1493)[0][0x64](IO  2) is 0x0000, (0,0)
Peek(DFX0000/1493)[0][0x70](INT 0) is 0x0C02, (12,2)
Peek(DFX0000/1493)[0][0x74](DMA 0) is 0x04, (4)
Peek(DFX0000/1493)[0][0x74](DMA 0) is 0x04, (4)
Peek(DFX0000/1493)[0][0x40](MEM 0) is 0x0000000000000000, (0,0,0,0,0,0,0,0)
Peek(DFX0000/1493)[0][0x60](-REG-) is 0x03, (3)
Peek(DFX0000/1493)[0][0x61](-REG-) is 0xE8, (232)
Peek(DFX0000/1493)[0][0x62](-REG-) is 0x00, (0)
Peek(DFX0000/1493)[0][0x63](-REG-) is 0x00, (0)
Peek(DFX0000/1493)[0][0x64](-REG-) is 0x00, (0)
Peek(DFX0000/1493)[0][0x65](-REG-) is 0x00, (0)
Peek(DFX0000/1493)[0][0x70](-REG-) is 0x0C, (12)
Peek(DFX0000/1493)[0][0x71](-REG-) is 0x02, (2)
Peek(DFX0000/1493)[0][0x74](-REG-) is 0x04, (4)
Peek(DFX0000/1493)[0][0x75](-REG-) is 0x04, (4)

Bugs
====
I haven't tested the Memory setting stuff, as I haven't
got a card with suitable drivers. If it doesn't work, tell me,
and work around using poke, which I have tested.

The config option to pnpdump is experimental, and
doesn't always produce non-conflicting output.

Newer PCs don't always work, I now think this is due to faulty
hardware, see the FAQ for details.

Note
====
These programs must run as root, as they need unrestricted access
to the computer IO addresses. This could cause lots of problems,
so use with care. DO NOT MAKE THESE PROGRAMS SUID root !

This is particularly important now that pnpdump (with certain options)
uses popen() to invoke external programs.

Copyright
=========
These programs are copyright P.J.H.Fox (fox@roestock.demon.co.uk)
and distributed under the GPL (see COPYING).

If mailing patches, bug reports or comments, please put 'isapnp'
somewhere in the subject line, and mail to isapnp@roestock.demon.co.uk.

Warranty
========
There is NO WARRANTY for these programs.

These programs have been compiled on my machine using gcc 2.7.2.3,
flex 2.5.4 and linux 2.0.36, with libc-5.4.44 and they seem to work
for me.

However, due to the nature of these programs, they are very likely
to completely screw up your computer: USE AT YOUR OWN RISK. But if
you find them useful, or have some suggestions for improvement,
please tell me.

Credits
=======
Thanks to the following for bug reports, fixes, improvements and
suggestions for improvement to isapnptools.

Bob Clark <rlc@hrb.com>
Neal Sanche <neal@nsdev.ocunix.on.ca>
Karsten Keil <pnp@temic-ech.spacenet.de>
Jim Studt <jim@federated.com)
Kevin Brooks <kb10@onyx.net>
Jeff Epler <jepler@inetnebr.com>
Markus Gutschke <gutschk@uni-muenster.de>
Andy Sewell <puck@pookhill.demon.co.uk>
Rildo Pragana <rpragana@acm.org>
Richard Henderson <rth@cygnus.com>
Kai Dupke <dupke@koma.han.de>
Ken Walsby <kwalsby@ttransit.co.uk>
Rick van Rein <vanrein@cs.utwente.nl>
James S. Blachly <jblachly@ns.insolwwb.net>
Steffen Kremser <kremser@nukunuku.swb.de>
Adam J. Richter <adam@yggdrasil.com>
Norbert Klasen [ELSA AG] <support@elsa.de>
Colin Plumb <colin@nyx.net>
Robert Ekl <rekl@megsinet.net>
Hidetaka Hikashi <hikashi@mlb.co.jp>
Hetz Benhamou <hetz@isdn.net.il>
Rick van Rein < vanrein@cs.utwente.nl>
Jeffrey Hutzelman <jhutz+@cmu.edu>
Pavel Roskin <pavel_roskin@geocities.com>
Eugene <bom@classic.iki.rssi.ru>

See also
========

Users of isapnptools may be interested in the pnp mailing list
(pnp-list@redhat.com): To subscribe to the mailinglist, simply send a
message with the word "subscribe" in the Subject: field to
pnp-list-request@redhat.com. This list does seem rather quiet now
though.

Latest information of isapnptools is available at the time of writing
on my website: http://www.roestock.demon.co.uk/isapnptools/. This
includes an FAQ, and the htmlised manual pages, so please refer to this
first in the event of any difficulties.

Peter Fox
14-Feb-1999
