Wed May 19 13:24:39 1999  Martin Mares  <mj@albireo.ucw.cz>

	* Released the whole package as version 2.0.

Fri May 14 22:42:02 1999  Martin Mares  <mj@albireo.ucw.cz>

	* pci.ids: Added several new ID's contributed by people
	on the linux-pci list.

Mon Apr 19 15:21:08 1999  Jakub Jelinek  <jj@ultra.linux.cz>

	* lspci.c: Display I/O addresses correctly on sparc64.
	* lib/header.h: Ditto.

	* lib/configure: On sparc set HAVE_64BIT* as well, we want
	a binary which works on both 32bit and 64bit SPARCs.

Sun Apr 18 21:14:58 1999  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.c, lib/proc.c: Alpha compilation fixes from Matthew Jacob
	<mjacob@feral.com>.

	* pci.ids: A lot of updates from Adam J. Richter <adam@yggdrasil.com>.

Sun Feb 28 22:26:21 1999  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.c (do_map_bus): Don't dump functions 1--7 if not flagged
	as a multi-function device, because several single-function devices
	don't decode the function bits at all.

Sun Feb 14 23:48:22 1999  Martin Mares  <mj@albireo.ucw.cz>

	* Makefile (install): Don't use "-o root -g root" for installation
	since it breaks on machines where programs are not installed by root.
	Reported by Richard Gooch <rgooch@atnf.csiro.au>

Tue Feb  9 15:54:39 1999  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.c (show_bases): Use new address masking macros and pciaddr_t.

	* lib/pci.h: Using pciaddr_t for bus addresses, which are 32-bit
	or 64-bit depending on CPU.

	* lib/pci.h (PCI_ADDR_MEM_MASK): Added macros for address masks
	according to bus address width.

Thu Jan 28 20:54:16 1999  Martin Mares  <mj@albireo.ucw.cz>

	* Released as 1.99.4.

	* lspci.c: Capability list parser now recognizes both AGP
	registers and PCI Power Management registers (the latter
	is mainly guesswork based on DEC/Intel 21153 bridge specs
	since I don't have the PCI Power Management document).

	* lspci.c: Replaced numerous occurences of (x & flag) ? '+' : '-'
	by FLAG macro.

	* lspci.c: Added bridge checks to bus mapping code.

Wed Jan 27 14:59:16 1999  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.c: Implemented bus mapping mode (-M).

	* lspci.c (scan_devices): Split to scan_devices() and scan_device().
	(show): Split to show() and show_device().

	* lib/access.c (pci_init): When a->method == PCI_ACCESS_AUTO,
	set it to the real access method afterwards.

Mon Jan 25 23:46:13 1999  Martin Mares  <mj@albireo.ucw.cz>

	* lib/generic.c (pci_generic_fill_info): If in buscentric mode,
	don't check PCI_COMMAND for I/O and memory enables.

Mon Jan 25 21:28:49 1999  Martin Mares  <mj@albireo.ucw.cz>

	* Makefile: Added target `release' which substitutes new version
	number to .spec, .lsm and README. Also rewrote target `dist'.

	* Released as 1.99.3.

Sun Jan 24 22:10:36 1999  Martin Mares  <mj@albireo.ucw.cz>

	* lib/header.h: Until kernel adopts new layout of PCI
	includes (i.e., separate declaration of header structure,
	functions and device IDs), which is not going to happen
	before 2.3, we'll use our own definiton of the header.

	* lspci.c (show_verbose): Display `Cap' flag in device status.

	* lspci.c (show_htype0): Display capability lists whereever
	available. The only capability name we recognize now is `AGP'.
	Unfortunately, capabilities are stored in device-dependent
	portion of the configuration space and are thus available
	only to root unless you read a dump.

	* lspci.c (scan_devices): Use cache instead of buffering.

	* lib/buffer.c: Removed (obsoleted by the cache).

	* lib/access.c: Added general caching mechanism.

Sat Jan 23 21:30:54 1999  Martin Mares  <mj@albireo.ucw.cz>

	* pci.ids: Added few devices.

Fri Jan 22 19:29:31 1999  Martin Mares  <mj@albireo.ucw.cz>

	* Version string is now defined in top-level Makefile, exported
	to the configure script and also substituted to man pages.

	* lspci.c (show_bases): Rewrote displaying of 64-bit addresses.
	(show_verbose): Rewrote interrupt display logic.

	* lib/i386-ports.c: Include sys/io.h only on glibc systems.

	* lib/configure: Rewrote detection of Linux versions. Now it
	works on 2.0 kernels (only with direct/dump access, of course).

	* lib/internal.h: New bytesex macros using <asm/byteorder.h>
	whenever available.

	* lib/proc.c (proc_read, proc_write): Distinguish between short
	read/write and real errors.

	* lspci.c (show_htype{0,1}): Always use d->dev->rom_base_addr since
	libpci respects buscentric mode automatically.

	* lspci.c (show_hex_dump): For CardBus bridges, print out 128
	bytes of header (the whole standard part).

	* common.c: pcilib options are now all uppercase. Also moved
	PCI access debugging option here.

	* Released as 1.99.2.

Wed Jan 20 22:50:35 1999  Martin Mares  <mj@albireo.ucw.cz>

	* Wrote configure script and rewrote Makefiles.

	* Removed few unused variables.

Wed Jan 20 12:21:56 1999  Martin Mares  <mj@albireo.ucw.cz>

	* common.c: Moved several functions used in both setpci and lspci
	here. This includes parsing of libpci-related options.

	* More library tweaks.

	* filter.c, names.c: Moved to library.

	* setpci: Rewritten to use the library.

	* Released as 1.99.1.

Tue Jan 19 23:00:12 1999  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.c (scan_devices): For cardbus bridges, read first 128
	bytes of config space to get full standard header.

	* Makefile (CFLAGS): Removed "-Wno-unused".

	* Started the "New Generation" branch and introduced the
	PCI library.
	
	* lspci: Rewritten to use the library.

Tue Jan 19 22:24:08 1999  Martin Mares  <mj@albireo.ucw.cz>

	* Released as version 1.10.

Mon Jan 18 08:51:17 1999  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.8, setpci.8: Miscellaneous fixes as suggested by
	Dag Wieers <dag@digibel.be>.

Sun Nov 29 20:05:56 1998  Martin Mares  <mj@albireo.ucw.cz>

	* pciutils.spec (Name): Update from Krzysztof G. Baranowski.

Sun Nov 22 10:49:56 1998  Martin Mares  <mj@albireo.ucw.cz>

	* Makefile, pciutils.h: Moved pci.ids to /usr/share.

	* Released as version 1.09.

Wed Nov 18 15:47:05 1998  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.c (show_htype1): Fixed displaying of prefetchable memory behind
	bridge. Thanks to Petr Vandrovec <vandrove@vc.cvut.cz> for bug report.

Fri Oct 23 18:59:19 1998  Martin Mares  <mj@albireo.ucw.cz>

	* setpci.c: Don't include <syscall-list.h> with glibc >= 2.1.

Mon Oct 19 21:53:30 1998  Martin Mares  <mj@albireo.ucw.cz>

	* Released as version 1.08.

	* setpci.c: glibc 2.1.x already defines pread() and pwrite().

	* lspci.8: Changed warning about lspci -xxx.

	* lspci.c: Require "-xxx" for full configuration space dump, so that
	it's impossible to crash the machine by single typo.

	* specs: Added (courtesy of Krzysztof G. Baranowski <kgb@knm.org.pl>).

Wed Sep  9 12:03:24 1998  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.c (show_bases): Better displaying of unassigned and
	disabled bases. Thanks to Gabriel Paubert <paubert@iram.es>
	for an idea.

Wed Sep  2 10:58:01 1998  Martin Mares  <mj@albireo.ucw.cz>

	* setpci.c (pread): Recognize glibc 1.99 numbered as 2.0 on the PPC.
	(thanks to Geert Uytterhoeven for finding this out)

Fri Jul 17 10:43:30 1998  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.c (show_verbose): Print subsystem ID using the new resolver.
	(show_machine): Print subsystem ID.

	* names.c: New name resolution engine supporting subsystem IDs.

	* Released as version 1.07.

Wed Jul 15 15:37:21 1998  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.c (show_htype2 etc.): Displaying of CardBus headers.
	(show_bases): Honor the `cnt' argument.
	(grow_tree): Parse CardBus headers in tree mode as well.

	* pci.h: Updated CardBus header field description. I still don't
	have the CardBus standard available, but OZ6832 specs contain
	full description of all header fields supported by the chip.

Tue Jun  9 22:53:59 1998  Martin Mares  <mj@albireo.ucw.cz>

	* Released as 1.06.

	* names.c (parse_name_list): Killed an unused variable.

	* setpci.c (pread, pwrite): Define SYS_(pread|pwrite) as __NR_\1
	if they are not defined by glibc (needed for glibc built on older
	kernels). Ugly.

	* setpci.c (exec_op): Fixed error messages. Thanks, Steve!

Mon Jun  8 10:59:22 1998  Martin Mares  <mj@albireo.ucw.cz>

	* Released as 1.05.

	* setpci.c: Problems with pread()/pwrite() with glibc on Alpha
	should be gone. Again thanks to Steve for bug report.

	* filter.c (filter_parse_slot): Fixed ":x" type filters.

	* pci.ids: Killed duplicate entry. Thanks to Stephen Williams
	<steve@icarus.com> for reporting this.

Sun Jun  7 19:27:51 1998  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.c (main), setpci.c (main): Implemented "--version".

	* Released as 1.04.

	* pciutils.h (PCIUTILS_VERSION): Added version string.

	* filter.c, names.c: Extraneous #include <linux/pci.h> removed.
	Thanks to Geert Uytterhoeven <Geert.Uytterhoeven@cs.kuleuven.ac.be>
	for bug report.

Thu May 28 14:45:58 1998  Martin Mares  <mj@lomikel.karlin.mff.cuni.cz>

	* pci.ids: More updates from Jens Maurer.

Wed Apr 22 10:00:39 1998  Martin Mares  <mj@albireo.ucw.cz>

	* pci.ids: Updates from Jens Maurer.

Sun Apr 19 11:14:25 1998  Martin Mares  <mj@albireo.ucw.cz>

	* Released as 1.03.

	* setpci.8: Written.

	* setpci.c: Finished.

	* lspci.c: Now able to fetch expansion ROM base from kernel device list
	and print it if not in buscentric mode.

Tue Mar 31 23:11:57 1998  Martin Mares  <mj@albireo.ucw.cz>

	* setpci.c: Added.

Sun Mar 22 15:39:08 1998  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.8: Updated the documentation.

	* lspci.c: Modified to use the new filtering mechanism (options -f and -d).

	* filter.c: Introduced new generic device filter.

Thu Mar 19 17:03:48 1998  Martin Mares  <mj@lomikel.karlin.mff.cuni.cz>

	* lspci.c (grow_tree, show_tree_dev, print_it): Fixed displaying
	of PCI-to-PCI bridges in the tree format.

Sun Feb 15 10:12:25 1998  Martin Mares  <mj@albireo.ucw.cz>

	* lspci.c (show_machine): Added non-verbose mode of machine-readable
	dump.

	* pci.ids: Updates from Jens Maurer.

	* Released as version 1.02.

Thu Feb 12 16:53:28 1998  Martin Mares  <mj@lomikel.karlin.mff.cuni.cz>

	* lspci.c: Added a "-m" switch for dumping machine-readable
	configuration data (requested by Bjoern Kriews <bkr@cut.de>).

Mon Feb  9 13:17:43 1998  Martin Mares  <mj@albireo.ucw.cz>

	* Makefile, pciutils.h: Include local pci.h instead of <linux/pci.h>
	if available. This should avoid all problems with official kernel
	not synchronized to newer PCI code in CVS -- standard distribution
	of pciutils now contains pci.h from current CVS kernel, pciutils
	in CVS contain no pci.h and use the correct kernel include.

	* Makefile: Fixed installation path for man pages.

Sat Feb  7 15:15:46 1998  Martin Mares  <mj@albireo.ucw.cz>

	* README: Updated.

	* lspci.8: Created a man page.

	* Releasing as version 1.0.

Tue Feb  3 20:56:00 1998  Martin Mares  <mj@albireo.ucw.cz>

	* Makefile: Recognize architecture by calling uname and pass it as ARCH_xxx
	to all the C sources. This should eliminate problems with 32-bit compilers
	on sparc64.

	* lspci.c (show_verbose): Recognize CardBus bridge header type.
	(show_htype2): Stub routine.
	(scan_config): Write sensible error message if the kernel denies reading of
	upper part of the PCI config space.

