
README.ppa (c) 1996   Grant R. Guenther,  grant@torque.net


         The IOMEGA PPA3 parallel port SCSI Host Bus Adapter

                     as embedded in the ZIP drive


This README documents the Linux support for the parallel port version of
IOMEGA's ZIP100.  The ZIP100 is an inexpensive and popular, but relatively 
low performance, removable medium disk device.  The drive is also available
as a regular SCSI device, but the driver documented here is for the
parallel port version.  IOMEGA implemented the parallel port version by
integrating (or emulating ?) their PPA3 parallel to SCSI converter into
the ZIP drive.

I have implemented a low-level driver, ppa.c,  for this parallel port 
host bus adapter, thereby supporting the parallel port ZIP drive as a 
regular SCSI device under Linux.

It is possible that this driver will also work with the original PPA3
device (to access a CDrom, for instance). But, the PPA3 is hard to find 
and costs as much as the ZIP drive itself, so no-one has actually tried
this, to the best of my knowledge.

The driver was developed without the benefit of any technical specifications 
for the interface.  Instead, a modified version of DOSemu was used to 
monitor the protocol used by the DOS driver, 'guest.exe', for this adapter.
I have no idea how my programming model relates to IOMEGA's design.
(One technical consequence of this method:  I have never observed a
SCSI message byte in the protocol transactions between guest.exe and
the ZIP drive, so I do not know how they are delivered.  My working 
hypothesis is that we don't have to worry about them if we don't
send linked commands to the drive.)

I'd like to thank Byron Jeff (byron@cc.gatech.edu) for publishing his
observation that the 'guest' driver loads under DOSemu.  His remark was
the stimulus that began this project.

The ppa driver can detect and adapt to 4- and 8-bit parallel ports, but 
there is currently no support for EPP or ECP ports, as I have been unable 
to make the DOS drivers work in these modes on my test rig.

The driver may be built in to the kernel, or loaded as a module.  It
may be configured on the command line in both cases, although the syntax
is different.  It may also be configured by editing the source file.

Built-in drivers accept parameters using this LILO/LOADLIN command line
syntax (omitted parameters retain their default values):

        ppa=base[,speed_high[,speed_low[,nybble]]]

For example:    ppa=0x378,0,3

If a driver is loaded as a module the parameters may be set on the
insmod command line, but each one must be specified by name:

For example:    insmod ppa.o ppa_base=0x378 ppa_nybble=1

(Notice the ppa_ prefix on each of the parameters in the insmod form.)

Here are the parameters and their functions:

Variable        Default    Description

ppa_base        0x378   The base address of PPA's parallel port.
ppa_speed_high  1       Microsecond i/o delay used in data transfers
ppa_speed_low   6       Microsecond delay used in other operations
ppa_nybble      0       1 to force the driver to use 4-bit mode.

A word about the timing parameters:  the ppa_speed_low parameter controls 
the widths of a large number of pulses that are sent over the parallel bus, 
the narrower the pulses, the faster things go, but the greater the risk of 
distortion by noise damping circuits in the parallel ports.  The 
ppa_speed_high parameter controls the same delays, but during the data 
transfer phase only.   In this phase, there is a lot of handshaking going 
on and the pulse shaping should not be so much of an issue, but if you 
see data corruption, you can increase this parameter as well.

You might also want to reduce the timing values to attempt to increase
the transfer rates on your system.  Please be careful to watch for
SCSI timeout errors in your log files.  If you are getting timeouts, you
have set these parameters too low.  The default values appear to be
safe on most machines.

If you have both the lp and ppa drivers in your kernel, you must ensure
that they access different parallel ports.  By default, the lp driver is
initialised early in the booting process, and it claims all parallel
ports that it can find.  You may control this behaviour with a LILO or
LOADLIN command line argument of the form:

        lp=base0[,irq0[,base1[,irq1[,base2[,irq2]]]]]

For example:    lp=0x278,7

If you use this method, only the ports named will be adopted by the lp
driver.  You can disable them all with lp=0 .

So, if you have a printer on 0x3bc and a ZIP drive on 0x278 you would
give the following options on your boot command:

        lp=0x3bc ppa=0x278

In this case lp would use the polling driver, since an interrupt was not 
specified.

If you want to share the same parallel port between a ZIP drive and a
printer, you should build both the lp and ppa drivers as modules and
load and unload one or the other as required.  This is clumsy but we
currently have no protocol for synchronising access to shared parallel
ports.

For information about using the ZIP drive, please read the generic
instructions in the SCSI-HOWTO and the man pages for the normal disk
management tools,  fdisk, mkfs, mount, umount, etc.  There is a mini-HOWTO
circulating concerning the use of the normal SCSI version of the ZIP
drive, most of its comments will apply to disks connected through the
ppa driver as well.



********************************************************
-------- Terse where to get ZIP Drive help info --------

General Iomega ZIP drive page for Linux:
http://www.torque.net/~campbell/

Driver achive for old drivers:
http://www.torque.net/~campbell/ppa/

Linux Parport page (parallel port)
http://www.torque.net/parport/

Email list for Linux Parport
linux-parport@torque.net

Email for problems with ZIP or ZIP Plus drivers
campbell@torque.net
********************************************************
