	Pcmcia Wireless configuration
	-----------------------------

	One of the most exciting thing having happen after release 20
is the addition of Wireless Extension support in the Pcmcia init
scripts. Here is a quick intro on the subject...

Pre-requisite :
-------------
	o Pcmcia package with Wireless Extension support : 3.1.15 onward
	o A driver with Wireless Extension support
	o The tools (iwconfig and co.) installed in the /usr/local/sbin
		or /usr/sbin

Raylink driver :
--------------
	The Raylink driver as of 1.70 doesn't support yet writable
Wireless Extensions, so enabling wireless.opts on this driver will
make thing worse.
	On the other hand, the latest version of the Raylink driver
accept Wireless Extensions at boot time, so the procedure described
below will work.

Distribution specific notes :
---------------------------
	Most modern distributions don't use wireless.opts and have
their own procedure for wireless configuration, which is usually
compatible with their configuration tools and work for non-Pcmcia
devices. This is documented in DISTRIBUTIONS.txt.
	The procedure described here will work only with the original
Pcmcia configuration scripts. If you use a precompiled package part of
a distributions, this is usually not the case (see above).
	On the other hand, if you install the Pcmcia package in source
form from the official Linux-Pcmcia web site, it will install the
proper init scripts and those instructions will apply.

Basic support :
-------------
	The file /etc/pcmcia/wireless.opts contain some templates for
the most common drivers. Just fill in your card configuration in the
template corresponding to your driver configuration.
	Then, to activate it, you just need to remove or comment the 4
lines at the top of wireless.opts and restart the Pcmcia package.

	Things to take care of :
	The options of wireless.opts will be used directly as
arguments of iwconfig. So, you need iwconfig, and you need to check
the man page of iwconfig to know how to format them.
	A quick way to determine the correct options without
restarting Pcmcia is to play a bit with iwconfig directly to see what
is possible and what is the proper setup of the card and to copy that
in wireless.opts.
	At the end of wireless.opts, there is also a generic template
containing all the possible options and explaining their meaning. Not
all of them are supported by all cards (actually, most cards support a
limited subset of it).
	The current card templates are designed to match the MAC
address of the card. Please check that this matches with your card.
	Also, sample describe the most common/useful options available
with the card, for more advance option, borrow options from the
template. You can also remove some options, the card will usually
initialise with a sane value.

	Alternatively, you can also discard the current wireless.opts
and replace it with a file looking like this :
----------- wireless.opts ---------------------
case "$ADDRESS" in
*,*,*,*)
    ESSID="MY_ESSID"
    MODE="Managed"
    ;;
esac
-----------------------------------------------


Scheme support :
--------------
	The file wireless.opts fully support schemes. This allow you
to define different configurations (home, work...) and to switch on
the fly between them.
	The best way to explain it is to show an example.
	Let's say you have an infrastructured setup at work (MY_WORK)
and an adhoc network at home (MY_HOME). Moreover, when a specific card
is inserted, you want it to be in adhoc mode (TEST). The work setup
will be the default...

	Each Wireless LAN will have the following configuration :
--------- wireless.opts --------------------
# Lucent Wavelan IEEE - Ad-Hoc mode for test card
*,*,*,00:60:1D:03:9F:2D)
    ESSID="TEST"
    MODE="Ad-Hoc"
    FREQ="10"
    RATE="1M"
    ;;

# Lucent Wavelan IEEE - Ad-Hoc mode at home
home,*,*,00:60:1D:*|home,*,*,00:02:2D:*)
    ESSID="MY_HOME"
    MODE="Ad-Hoc"
    FREQ="5"
    ;;

# Lucent Wavelan IEEE - infrastructured mode at work
*,*,*,00:60:1D:*|*,*,*,00:02:2D:*)
    ESSID="MY_WORK"
    MODE="Managed"
    KEY="s:verysecurekey"
    ;;
--------------------------------------------

	Don't forget the IP configuration :
--------- network.opts ---------------------
# Wavelan IEEE : ad-hoc mode for test card
*,*,*,00:60:1D:03:9F:2D)
    DHCP="n"
    IPADDR="10.0.0.1"
    NETMASK="255.255.255.0"
    NETWORK="10.0.0.0"
    BROADCAST="10.0.0.255"
    ;;

# Wavelan IEEE : ad-hoc mode at home
home,*,*,00:60:1D:*|home,*,*,00:02:2D:*)
    DHCP="n"
    IPADDR="10.0.1.19"
    NETMASK="255.255.255.0"
    NETWORK="10.0.1.0"
    BROADCAST="10.0.1.255"
    GATEWAY="15.0.1.1"
    ;;

# Wavelan IEEE : infrastructured mode at work
*,*,*,00:60:1D:*|*,*,*,00:02:2D:*)
    DHCP="y"
    ;;
--------------------------------------------

	Now, when you are at work you do :
> cardctl scheme default
	And at home, you do :
> cardctl scheme home

	I guess you get the idea ;-)

More elaborated configurations :
------------------------------
	Some people may need some more complex configurations. For
example, you might want to do one of the following thing :
		o cycle through a set of schemes
		o autodetect the proper scheme
	There is currently no support to do that. However, the
Wireless Tools package contains a tool called "iwgetid" that can help
in this job. The source code contains some hints on how to achieve the
above thing.
	If you ever write such a package, please send me the URL.
	Good luck !


	Jean <jt@hpl.hp.com>
