You need to have at least Openserver 5.0.4 in order to
use cdrecord.

On SCO Openserver, there is no support for cdrecord -scanbus

As there is no real generic SCSI driver, cdrecord uses the
pass through ioctl of the cdrom driver.

The correct dev= syntax on SCO Openserver is:

dev=cdrom-device:target,lun

If you want to talk to the 2nd cdrom device which is in target 6, you
should use:

cdrecord dev=/dev/rcd1:6,0

To compile, you need 'smake' from:

	ftp://ftp.fokus.gmd.de/pub/unix/makefiles/bin/

or 'gmake'. Smake is preferred as gmake bugs will cause bogus warnings
and may confuse about the state of the make run.


Some general notes on cdrecord are on:

	http://www.sco.com/skunkware/cdrecord/SCO-NOTES.html

But note:

-	Do not change cdrecord-1.8a22 or later, it compiles without
	changes on SCO Openserver.

-	It is currently not possible to compile the actual source
	on SCO UnixWare. Get the 'skunkware' binary.
