<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Configuration</TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="i740.html"><EM>Information for i740 Users</EM></A>
 <b>:</b> <EM>Configuration</EM><BR>
<b>Previous:</b> <A HREF="i7404.html"><EM>Reported Working Video Cards</EM></A><BR>
<b>Next:</b> <A HREF="i7406.html"><EM>Driver Options</EM></A>


<HR NOSHADE>
  <H2><A NAME="5"></A>5. Configuration</H2>
<p>The driver auto-detects all device information necessary to
initialize the card.  The only lines you need in the "Device"
section of your XF86Config file are:
<pre>
       Section "Device"
           Identifier "i740"
       EndSection
</pre>

or let xf86config or XF86Setup do this for you.</p>
<p>However, if you have problems with auto-detection, you can specify:
<ul>
<li>VideoRam - in kilobytes</li>
<li>DacSpeed - in MHz</li>
<li>MemBase  - physical address of the linear framebuffer</li>
<li>IOBase   - physical address of the memory mapped IO registers</li>
</ul>
</p>


 <HR NOSHADE>
<A HREF="i740.html"><EM>Information for i740 Users</EM></A>
 <b>:</b> <EM>Configuration</EM><BR>
<b>Previous:</b> <A HREF="i7404.html"><EM>Reported Working Video Cards</EM></A><BR>
<b>Next:</b> <A HREF="i7406.html"><EM>Driver Options</EM></A>



</BODY>
</HTML>
