<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Basic configuration </TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="tseng.html"><EM> Information for Tseng Chipset Users</EM></A>
 <b>:</b> <EM>Basic configuration </EM><BR>
<b>Previous:</b> <A HREF="tseng6.html"><EM>Text mode restore problems </EM></A><BR>
<b>Next:</b> <A HREF="tseng8.html"><EM>general options in the <code>XF86Config</code> file </EM></A>


<HR NOSHADE>
  <H2><A NAME="7"></A>7. Basic configuration </H2>

<p>It is recommended that you generate an XF86Config file using
the <code>XF86Setup</code>' or <code>xf86config</code>' program, which should
produce a working
high-resolution 8bpp configuration. You may want to include mode
timings in the <code>Monitor</code> section that better fit your monitor
(e.g 1152x864 modes). The driver options are described in detail in
the next section; here the basic options are hinted at.</p>
<p>If graphics redrawing goes wrong on accelerated chips (ET4000W32 and
ET6000), first try the <code>"noaccel"</code> option, which disables
all accelerated functions.</p>


 <HR NOSHADE>
<A HREF="tseng.html"><EM> Information for Tseng Chipset Users</EM></A>
 <b>:</b> <EM>Basic configuration </EM><BR>
<b>Previous:</b> <A HREF="tseng6.html"><EM>Text mode restore problems </EM></A><BR>
<b>Next:</b> <A HREF="tseng8.html"><EM>general options in the <code>XF86Config</code> file </EM></A>



</BODY>
</HTML>
