<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Known Bugs </TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="P9000.html"><EM>XFree86 P9000 Server Release Notes</EM></A>
 <b>:</b> <EM>Known Bugs </EM><BR>
<b>Previous:</b> <A HREF="P900010.html"><EM>XF86Config </EM></A><BR>
<b>Next:</b> <A HREF="P900012.html"><EM>Credits </EM></A>


<HR NOSHADE>
  <H2><A NAME="14"></A>11. Known Bugs </H2>
<p>There are currently problems with the server when used in conjunction
with xdm, olvwm, and VT switching under Linux.  </p>
<p>If the cursor changes while you're in a VT, the cursor won't look
right when you return from the VT until it is moved between windows
(and changes color and shape).</p>
<p>Memory probing does not work.  You will need to explicitly specify the
amount of memory you have.  If you have a 1 MB card, try put
<code>VideoRAM 1024</code> into the <code>Device</code> section of your
<code>XF86Config</code> file.  If this doesn't work, try adding
<code>Option "vram_128"</code> to the <code>Device</code> section.</p>

 <HR NOSHADE>
<A HREF="P9000.html"><EM>XFree86 P9000 Server Release Notes</EM></A>
 <b>:</b> <EM>Known Bugs </EM><BR>
<b>Previous:</b> <A HREF="P900010.html"><EM>XF86Config </EM></A><BR>
<b>Next:</b> <A HREF="P900012.html"><EM>Credits </EM></A>



</BODY>
</HTML>
