<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Features:</TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="MGA.html"><EM>Information for Matrox Users</EM></A>
 <b>:</b> <EM>Features:</EM><BR>
<b>Previous:</b> <A HREF="MGA1.html"><EM>Supported hardware</EM></A><BR>
<b>Next:</b> <A HREF="MGA3.html"><EM>Configuration:</EM></A>


<HR NOSHADE>
  <H2><A NAME="3"></A>2. Features:</H2>
<p>
<ul>
<li>uses linear frame buffer</li>
<li>Resolutions up to the maximum supported by the card should be possible.</li>
<li>8 bpp, 16 bpp (depth 15 and 16), 24 bpp (depth 24, packed) and 32 bpp
(depth 24, sparse) are all supported.</li>
<li>supports VESA Display Power Management Signaling (DPMS)</li>
<li>supports RGB Sync-on-Green </li>
<li>supports the XF86_DGA extension</li>
<li>Makes extensive use of the graphics accelerator.  This server is very 
well accelerated, and is one of the fastest XFree86 X servers.</li>
</ul>
</p>

 <HR NOSHADE>
<A HREF="MGA.html"><EM>Information for Matrox Users</EM></A>
 <b>:</b> <EM>Features:</EM><BR>
<b>Previous:</b> <A HREF="MGA1.html"><EM>Supported hardware</EM></A><BR>
<b>Next:</b> <A HREF="MGA3.html"><EM>Configuration:</EM></A>



</BODY>
</HTML>
