<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Supported hardware</TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="I128.html"><EM>Information for Number Nine I128 Users</EM></A>
 <b>:</b> <EM>Supported hardware</EM><BR>
<b>Previous:</b> <A HREF="I128.html"><EM>Information for Number Nine I128 Users</EM></A><BR>
<b>Next:</b> <A HREF="I1282.html"><EM>Features:</EM></A>


<HR NOSHADE>
  <H2><A NAME="1"></A>1. Supported hardware</H2>
<p>The current accelerated I128 server supports</p>
<p>
<ul>
<li>Imagine 128
(I128 with Texas Instruments TVP3025 or IBM528 RAMDAC). It has been tested with 
with 4MB of VRAM. </li>
<li>Imagine 128 Ticket 2 Ride
(I128-T2R with IBM526 or 528 RAMDAC). It has been tested with 4 MB and 8 MB of
VRAM and DRAM.</li>
<li>Imagine 128 Revolution 3D
(I128-R3D with IBM526 RAMDAC).  It has been tested with 4 MB, 8 MB, and 16 MB
of WRAM or SGRAM.</li>
<li>Imagine 128 Revolution IV
(I128-R4 with SILVERHAMMER RAMDAC).  It has been tested with 32 MB.</li>
</ul>
</p>

 <HR NOSHADE>
<A HREF="I128.html"><EM>Information for Number Nine I128 Users</EM></A>
 <b>:</b> <EM>Supported hardware</EM><BR>
<b>Previous:</b> <A HREF="I128.html"><EM>Information for Number Nine I128 Users</EM></A><BR>
<b>Next:</b> <A HREF="I1282.html"><EM>Features:</EM></A>



</BODY>
</HTML>
