<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>List of Supported Clock Chips</TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="S3.html"><EM> Information for S3 Chipset Users</EM></A>
 <b>:</b> <EM>List of Supported Clock Chips</EM><BR>
<b>Previous:</b> <A HREF="S32.html"><EM>16bpp and 32bpp</EM></A><BR>
<b>Next:</b> <A HREF="S34.html"><EM>List of Supported RAMDAC Chips</EM></A>


<HR NOSHADE>
  <H2><A NAME="3"></A>3. List of Supported Clock Chips</H2>

<p>
<blockquote><code>
<pre>
ICD2061A                                ==&gt; ClockChip "icd2061a"
ICS9161A (ICD2061A compatible)          ==&gt; ClockChip "ics9161a"
DCS2824-0 (Diamond, ICD2061A comp.)     ==&gt; ClockChip "dcs2824"
 
S3 86c708 GENDAC                        ==&gt; ClockChip "s3gendac"
ICS5300 GENDAC (86c708 compatible)      ==&gt; ClockChip "ics5300"

S3 86c716 SDAC                          ==&gt; ClockChip "s3_sdac"
ICS5342 GENDAC                          ==&gt; ClockChip "ics5342"
STG 1703                                ==&gt; ClockChip "stg1703"
 
Sierra SC11412                          ==&gt; ClockChip "sc11412"
ICS2595                                 ==&gt; ClockChip "ics2595"
TI3025                                  ==&gt; ClockChip "ti3025"
TI3026                                  ==&gt; ClockChip "ti3026"
IBM RGB 5xx                             ==&gt; ClockChip "ibm_rgb5xx"

Chrontel 8391                           ==&gt; ClockChip "ch8391"

AT&amp;T 20C409				==&gt; ClockChip "att20c409"
AT&amp;T 20C499 (untested)		==&gt; ClockChip "att20c499"
</pre>
</code></blockquote>
</p>

 <HR NOSHADE>
<A HREF="S3.html"><EM> Information for S3 Chipset Users</EM></A>
 <b>:</b> <EM>List of Supported Clock Chips</EM><BR>
<b>Previous:</b> <A HREF="S32.html"><EM>16bpp and 32bpp</EM></A><BR>
<b>Next:</b> <A HREF="S34.html"><EM>List of Supported RAMDAC Chips</EM></A>



</BODY>
</HTML>
