<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Support chipsets</TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="apm.html"><EM> Information for Alliance Promotion chipset users</EM></A>
 <b>:</b> <EM>Support chipsets</EM><BR>
<b>Previous:</b> <A HREF="apm.html"><EM> Information for Alliance Promotion chipset users</EM></A><BR>
<b>Next:</b> <A HREF="apm2.html"><EM>Acceleration</EM></A>


<HR NOSHADE>
  <H2><A NAME="1"></A>1. Support chipsets</H2>
<p>The apm driver in the SVGA server is for Alliance Promotion
(www.alsc.com) graphics chipsets. The following chipsets are supported:</p>
<p>
<ul>
<li> 6422

Old chipset without color expansion hardware (text accel).
</li>
<li> AT24

As found in Diamond Stealth Video 2500. Quite similar to AT3D.
</li>
<li> AT25, AT3D

AT3D is found in Hercules Stingray 128/3D. Most other Voodoo
Rush based cards use the AT25 which is identical except it
doesn't have the 3D stuff in it.</li>
</ul>
</p>

 <HR NOSHADE>
<A HREF="apm.html"><EM> Information for Alliance Promotion chipset users</EM></A>
 <b>:</b> <EM>Support chipsets</EM><BR>
<b>Previous:</b> <A HREF="apm.html"><EM> Information for Alliance Promotion chipset users</EM></A><BR>
<b>Next:</b> <A HREF="apm2.html"><EM>Acceleration</EM></A>



</BODY>
</HTML>
