<!DOCTYPE html PUBLIC "-//W3C//DTD HTML 3.2 Final//EN">
<HTML>
<HEAD>
<META HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=iso-8859-1">
<TITLE>Configuration</TITLE>
</HEAD>
<BODY BGCOLOR="#efefef" TEXT="black" LINK="blue" VLINK="#551A8B" ALINK="red">

<A HREF="neo.html"><EM> Information for NeoMagic Users 	            NeoMagic Driver Version 2.0.0</EM></A>
 <b>:</b> <EM>Configuration</EM><BR>
<b>Previous:</b> <A HREF="neo4.html"><EM>Reported Working Laptops</EM></A><BR>
<b>Next:</b> <A HREF="neo6.html"><EM>Driver Options</EM></A>


<HR NOSHADE>
  <H2><A NAME="5"></A>5. Configuration</H2>
<p>The driver auto-detects all device info included memory size, so
use the following device section in your XF86Config file:
<pre>
	Section "Device"
		Identifier	"NeoMagic"
	EndSection
</pre>

or let xf86config or XF86Setup do this for you.</p>
<p>But if you have problems with auto-detection, you can specify:
<pre>
      VideoRam  - in kilobytes
      DacSpeed  - in MHz
      MemBase   - physical address of the linear framebuffer
      MMIOBase  - physical address of the memory mapped IO registers
</pre>
</p>

 <HR NOSHADE>
<A HREF="neo.html"><EM> Information for NeoMagic Users 	            NeoMagic Driver Version 2.0.0</EM></A>
 <b>:</b> <EM>Configuration</EM><BR>
<b>Previous:</b> <A HREF="neo4.html"><EM>Reported Working Laptops</EM></A><BR>
<b>Next:</b> <A HREF="neo6.html"><EM>Driver Options</EM></A>



</BODY>
</HTML>
