                     Information for ATI Rage 128 Users

                     Precision Insight, Inc., SuSE GmBH

                               6 October 1999

1.  Supported Hardware

   o ATI Rage 128 based cards

2.  Features

   o Full support (including hardware accelerated 2D drawing) for 8, 15, 16,
     24, and 32 bit per pixel depths.

   o Hardware cursor support to reduce sprite flicker.

   o Support for high resolution video modes up to 1800x1440 @ 70Hz.

   o Support for doublescan video modes (e.g., 320x200 and 320x240).

   o Support for gamma correction at all pixel depths.

   o Fully programmable clock supported.

   o Robust text mode restore for VT switching.

3.  Technical Notes

   o None

4.  Reported Working Video Cards

   o Rage Fury AGP 32MB

   o XPERT 128 AGP 16MB

   o XPERT 99 AGP 8MB

5.  Configuration

The driver auto-detects all device information necessary to initialize the
card.  The only lines you need in the "Device" section of your XF86Config
file are:

            Section "Device"
                Identifier "r128"
            EndSection

or let xf86config or XF86Setup do this for you.

However, if you have problems with auto-detection, you can specify:

   o VideoRam - in kilobytes

   o MemBase  - physical address of the linear framebuffer

   o IOBase   - physical address of the memory mapped IO registers

   o ChipID   - PCI DEVICE ID

6.  Driver Options

   o "hw_cursor" - request hardware cursor (default)

   o "sw_cursor" - software cursor only

   o "no_accel"  - software rendering only

   o "dac_8_bit" - use color weight 888 in 8 bpp mode (default)

   o "dac_6_bit" - use color weight 666 in 8 bpp mode (VGA emulation)

7.  Known Limitations

   o None

8.  Authors

   o Alan Hourihane alanh@fairlite.demon.co.uk

   o Rickard E. (Rik) Faith <faith@precisioninsight.com>

   o Kevin E. Martin <kevin@precisioninsight.com>

   o Dirk Hohndel <hohndel@suse.de>

This driver was donated to The XFree86 Project by:

         Precision Insight, Inc.
         Cedar Park, TX
         USA

it is based on earlier work donated to The XFree86 Project by:

         SuSE GmbH
         Schanzaekerstr. 10
         90443 Nuernberg
         Germany

http://www.precisioninsight.com -- http://www.suse.com

     Generated from XFree86: xc/programs/Xserver/hw/xfree86/doc/sgml/r128.sgml,v 1.1.2.1 1999/10/11 21:04:38 hohndel Exp $
     $PI: xc/programs/Xserver/hw/xfree86/doc/sgml/r128.sgml,v 1.2 1999/10/08 08:33:58 faith Exp $

